For 1990-2009 cars

### Removal Procedure

1. Turn OFF the ignition.
2. Note the position of the EVAP hoses for installation.
3. Disconnect the EVAP canister purge valve electrical connector and hoses.
4. Remove the bolt from the purge valve mounting bracket.
5. Remove the EVAP purge valve.

### Installation Procedure

1. Position the EVAP canister purge valve on the manifold.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolt and secure the EVAP canister purge valve.

Tighten
Tighten the purge valve retaining bolt to 10 (88 lb in).

3. Connect the purge valve electrical connector and the hoses.