For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Automatic Transmission Range Selector Lever Screw | 20 N·m | 14 lb ft
Intermediate Shaft Bolt | 48 N·m | 35 lb ft
Steering Column Cover Bolts | 4 N·m | 38 lb in
Steering Column Bolts | 24 N·m | 18 lb ft
Steering Column Nuts | 24 N·m | 18 lb ft
Steering Wheel Nut * | 45 N·m | 33 lb ft
Turn Signal and Multifunction Lever Bolts/Screws | 6 N·m | 53 lb in
* This is a prevailing torque type fastener. This fastener may be reused ONLY if:

• | The fastener and its counterpart are clean and free from rust

• | The fastener develops a specified amount of torque (drag) against its counterpart prior to the fastener seating.

| Refer to the appropriate service procedure for the prevailing toque value.

If the fastener does not meet these criteria, REPLACE the fastener.