For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Booster Nut * | 25 N·m | 18 lb ft
Brake Hose Bolt at Front Brake Caliper | 54 N·m | 40 lb ft
Brake Hose Bolt at Rear Brake Caliper (Export Only) | 43 N·m | 32 lb ft
Brake Pedal Brace Nut | 10 N·m | 89 lb in
Brake Pedal Brace Bolt | 10 N·m | 89 lb in
Brake Pedal Bracket Nut | 5 N·m | 44 lb in
Brake Pipe Fitting | 21 N·m | 15 lb ft
* This is a prevailing torque type fastener. This fastener may be reused ONLY if:

• | The fastener and its counterpart are clean and free from rust

• | The fastener develops a specified amount of torque (drag) against its counterpart prior to the fastener seating.

| Refer to the appropriate service procedure for the prevailing torque value.

If the fastener does not meet these criteria, REPLACE the fastener.