For 1990-2009 cars

## Intake Manifold Removal Upper

1. Disconnect the MAP sensor electrical connector.
2. Remove the MAP sensor screws.
3. Remove the MAP sensor.
4. Remove the EGR valve pipe from the exhaust manifold.
5. Remove the EGR valve bolts.
6. Remove the EGR valve and gasket.
7. Remove the EGR valve pipe and gasket.
8. Remove the upper intake manifold studs and bolts.
9. Remove the upper intake manifold.
10. Remove the upper intake manifold gaskets.
11. Remove the upper intake manifold gaskets.

## Intake Manifold Removal Lower

1. Remove the fuel feed and return pipe retaining clip bolt.
2. Remove the fuel feed and return pipe retaining clip.
3. Remove the fuel injector rail bolts.
4. Remove the fuel injector rail assembly.
5. Remove the heater inlet pipe nut.
6. Remove the heater inlet pipe.
7. Remove the lower intake manifold bolts.
8. Remove the lower intake manifold.