For 1990-2009 cars

#### In-line Connector C101

Connector Part Information |

• | 12193583

• | 20-Way F Micro-Pack 100 W Series (GRY)

Connector Part Information

• | 12160542

• | 20-Way M Micro-Pack 100 W Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 882 | Wheel Speed Sensor Signal-Right Rear | A | BRN | 882 | Wheel Speed Sensor Signal-Right Rear
B | WHT | 883 | Wheel Speed Sensor Return-Right Rear | B | WHT | 883 | Wheel Speed Sensor Return-Right Rear
C | BLK | 884 | Wheel Speed Sensor Signal-Left Rear | C | BLK | 884 | Wheel Speed Sensor Signal-Left Rear
D | RED | 885 | Wheel Speed Sensor Return-Left Rear | D | RED | 885 | Wheel Speed Sensor Return-Left Rear
E | DK GRN/WHT | 762 | A/C Request Signal | E | DK GRN/WHT | 762 | A/C Request Signal
F | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | F | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
G | WHT | 1310 | Canister Vent Valve Solenoid Output | G | WHT | 1310 | Canister Vent Valve Solenoid Output
H | LT BLU | 1122 | Class 2 Serial Data Communication | H | LT BLU | 1122 | Class 2 Serial Data Communication
J | BLK | 2759 | Fuel Level Gauge Sensor Signal | J | BLK | 2759 | Fuel Level Gauge Sensor Signal
K | PPL | 1589 | Fuel Gauge Sensor Signal | K | PPL | 1589 | Fuel Gauge Sensor Signal
L | BRN/WHT | 1571 | Traction Control System Switch Signal | L | BRN/WHT | 1571 | Traction Control System Switch Signal
M | GRY | 2700 | Fuel Tank Pressure Sensor 5 Volt Reference | M | GRY | 2700 | Fuel Tank Pressure Sensor 5 Volt Reference
N | PPL | 806 | Fuse Output-Crank-Type 3 Fuse | N | PPL | 806 | Fuse Output-Crank-Type 3 Fuse
P | PNK | 1020 | Fuse Output-Off/RUN/Crank-Type 3 Fuse | P | PNK | 1020 | Fuse Output-Off/RUN/Crank-Type 3 Fuse
R | DK GRN | 1049 | Class 2 Serial Data Signal | R | DK GRN | 1049 | Class 2 Serial Data Signal
S | DK GRN | 83 | Cruise Control Signal-Disengage | S | DK GRN | 83 | Cruise Control Signal-Disengage
T | WHT | 85 | Cruise Control Indicator Lamp Output | T | WHT | 85 | Cruise Control Indicator Lamp Output
U | BRN/WHT | 419 | Check Engine Indicator Lamp Output | U | BRN/WHT | 419 | Check Engine Indicator Lamp Output
V | PPL | 420 | Brake Pedal Switch Output-Torque Converter Clutch | V | PPL | 420 | Brake Pedal Switch Output-Torque Converter Clutch
W | ORN/BLK | 434 | Transmission Mounted Neutral Safety Switch Signal | W | ORN/BLK | 434 | Transmission Mounted Neutral Safety Switch Signal

#### In-line Connector C102

Connector Part Information |

• | 15326084

• | 16-Way F GT Mixed Series Sealed (BLK)

Connector Part Information

• | 15326085

• | 16-Way M GT Mixed Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PNK | 639 | Fuse Output-Ignition 1-Type 3 Fuse | A | PNK | 639 | Fuse Output-Ignition 1-Type 3 Fuse
B | YEL | 410 | Coolant Temperature Sensor Signal | B | YEL | 410 | Coolant Temperature Sensor Signal
C | BLK | 1744 | Fuel Injector 1 Output | C | BLK | 1744 | Fuel Injector 1 Output
D | LT GRN/BLK | 1745 | Fuel Injector 2 Output | D | LT GRN/BLK | 1745 | Fuel Injector 2 Output
E | PNK/BLK | 1746 | Fuel Injector 3 Output | E | PNK/BLK | 1746 | Fuel Injector 3 Output
F | LT BLU/BLK | 844 | Fuel Injector 4 Output | F | LT BLU/BLK | 844 | Fuel Injector 4 Output
G | BLK/WHT | 845 | Fuel Injector 5 Output | G | BLK/WHT | 845 | Fuel Injector 5 Output
H | YEL/BLK | 846 | Fuel Injector 6 Output | H | YEL/BLK | 846 | Fuel Injector 6 Output
J | -- | -- | Not Used | J | -- | -- | Not Used
K | GRY | 2704 | MAP Sensor 5 Volt Reference | K | GRY | 2704 | MAP Sensor 5 Volt Reference
L | ORN/BLK | 469 | Manifold Absolute Pressure Sensor Return | L | ORN/BLK | 469 | Manifold Absolute Pressure Sensor Return
M | LT GRN | 432 | Manifold Absolute Pressure Sensor Signal | M | LT GRN | 432 | Manifold Absolute Pressure Sensor Signal
N | RED/WHT | 812 | Reference Voltage Feed-12 Volt Reference | N | RED/WHT | 812 | Reference Voltage Feed-12 Volt Reference
P | BLK | 407 | Sensor Return | P | BLK | 407 | Sensor Return
R | BLK | 630 | Camshaft Position Signal | R | BLK | 630 | Camshaft Position Signal
S | -- | -- | Not Used | S | -- | -- | Not Used

#### In-line Connector C105

Connector Part Information |

• | 12129565

• | 4-Way F Metri-Pack 280 Series Sealed (GRY)

Connector Part Information

• | 12129600

• | 4-Way M Metri-Pack 280 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 1050 | Ground | A | BLK | 1050 | Ground
B | LT BLU | 409 | Coolant Fan Motor Feed | B | LT BLU | 409 | Coolant Fan Motor Feed
C | GRY | 532 | Coolant Fan Motor Feed-Secondary | C | GRY | 532 | Coolant Fan Motor Feed-Secondary
D | WHT | 504 | Coolant Fan Motor Output | D | WHT | 504 | Coolant Fan Motor Output

#### In-line Connector C111

Connector Part Information |

• | 12160493

• | 14-Way F Micro-Pack 100 Series (GRY)

Connector Part Information

• | 12176566

• | 14-Way M Micro-Pack 100 W Lock Assist/ Seal (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | LT GRN | 1222 | 1-2 Shift Solenoid Valve Control | A | LT GRN | 1222 | 1-2 Shift Solenoid Valve Control
B | YEL/BLK | 1223 | 2-3 Shift Solenoid Valve Control | B | YEL | 1223 | 2-3 Shift Solenoid Valve Control
C | RED/BLK | 1228 | Pressure Control Solenoid Valve Controlled Power Feed | C | PPL | 1228 | Pressure Control Solenoid Valve Controlled Power Feed
D | LT BLU/WHT | 1229 | Pressure Control Solenoid Valve Controlled Ground | D | LT BLU | 1229 | Pressure Control Solenoid Valve Controlled Ground
E | PNK | 1339 | Fused Ignition 1 Feed | E | RED | 839 | Fused Ignition 1 Feed
L | YEL/BLK | 1227 | Transmission Temperature Sensor Signal | L | BRN | 1227 | Transmission Temperature Sensor Signal
M | BLK | 2762 | TFT Sensor Ground | M | GRY | 452 | TFT Sensor Ground
N | PNK | 1224 | TFP Switch Signal-A | N | PNK | 1224 | TFP Switch Signal-A
P | RED | 1226 | TFP Switch Signal-C | P | ORN | 1226 | TFP Switch Signal-C
R | DK BLU | 1225 | TFP Switch Signal-B | R | DK BLU | 1225 | TFP Switch Signal-B
S | RED/BLK | 1230 | Transmission Input Speed Sensor Signal | S | BLK | 1230 | Transmission Input Speed Sensor Signal
T | BRN | 418 | Torque Converter Clutch Solenoid Output | T | TAN | 418 | Torque Converter Clutch Solenoid Output
U | YEL | 657 | Torque Converter Clutch Release Switch Input | U | WHT | 1804 | Torque Converter Clutch Release Switch Input
V | DK BLU/WHT | 1231 | Transmission Input Speed Sensor Return | V | DK GRN | 1231 | Transmission Input Speed Sensor Return

#### In-line Connector C120

Connector Part Information |

• | 12110293

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Connector Part Information

• | 12129615

• | 3-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN/BLK | 735 | Ambient Air Temperature Sensor Signal | A | LT GRN/BLK | 735 | Ambient Air Temperature Sensor Signal
B | BLK | 1550 | Ground | B | BLK | 1550 | Ground
C | -- | -- | Not Used | C | -- | -- | Not Used

#### In-line Connector C171

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12162000

• | 2-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 873 | LF Wheel Speed Signal-Low | A | YEL | 873 | LF Wheel Speed Signal-Low
B | BLK | 830 | LF Wheel Speed Signal-High | B | LT BLU | 830 | LF Wheel Speed Signal-High

#### In-line Connector C172

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12162000

• | 2-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 833 | RF Wheel Speed Signal-Low | A | TAN | 833 | RF Wheel Speed Signal-Low
B | WHT | 872 | RF Wheel Speed Signal-High | B | DK GRN | 872 | RF Wheel Speed Signal-High

#### In-line Connector C200

Connector Part Information |

• | 12034257

• | 56-Way F Metri-Pack Mixed Series (BLK)

Connector Part Information

• | 12186339

• | 56-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | ORN | 340 | Fused Battery Feed | A1 | ORN | 340 | Fused Battery Feed
A2 | LT BLU | 1894 | Power Sliding Door Switch Signal | A2 | LT BLU | 1894 | Power Sliding Door Switch Signal
A3-A6 | -- | -- | Not Used | A3-A6 | -- | -- | Not Used
A7 | GRY | 120 | Fuel Pump Motor Feed | A7 | GRY | 120 | Fuel Pump Motor Feed
A8 | YEL | 143 | Fused Ignition 3 Feed | A8 | YEL | 143 | Fused Ignition 3 Feed
A9-B1 | -- | -- | Not Used | A9-B1 | -- | -- | Not Used
B2 | LT GRN | 275 | Transaxle Range Switch Feed-PARK | B2 | LT GRN | 275 | Transaxle Range Switch Feed-PARK
B3 | GRY/BLK | 690 | Courtesy Lamp Control | B3 | GRY/BLK | 690 | Courtesy Lamp Control
B4 | ORN | 1240 | Fused Battery Feed | B4 | ORN | 1240 | Fused Battery Feed
B6-B7 | -- | -- | Not Used | B6-B7 | -- | -- | Not Used
B8 | DK BLU | 1393 | Courtesy Lamps Feed-Protected Battery | B8 | DK BLU | 1393 | Courtesy Lamps Feed-Protected Battery
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
C1 | PPL | 328 | Interior Lamp Override Switch Output | C1 | PPL | 328 | Interior Lamp Override Switch Output
C2 | YEL | 1139 | Fused Ignition 1 Feed | C2 | YEL | 1139 | Fused Ignition 1 Feed
C3 | -- | -- | Not Used | C3 | -- | -- | Not Used
C4 | ORN | 267 | Heated Mirror Element Feed | C4 | ORN | 267 | Heated Mirror Element Feed
C6 | LT GRN/BLK | 735 | Ambient Air Temperature Sensor Signal | C6 | LT GRN/BLK | 735 | Ambient Air Temperature Sensor Signal
C7 | DK GRN | 389 | Vehicle Speed Signal (VSS) | C7 | DK GRN | 389 | Vehicle Speed Signal (VSS)
C8 | -- | -- | Not Used | C8 | -- | -- | Not Used
C9 | PNK | 1039 | Fused Igniton 1 Feed | C9 | PNK | 1039 | Fused Igniton 1 Feed
D1-D2 | -- | -- | Not Used | D1-D2 | -- | -- | Not Used
D3 | YEL | 743 | Fused Accessory Feed | D3 | YEL | 743 | Fused Accessory Feed
D6 | ORN | 1140 | Fused Battery Feed | D6 | ORN | 1140 | Fused Battery Feed
D7-D8 | -- | -- | Not Used | D7-D8 | -- | -- | Not Used
E1 | RED | 122 | Rear Fog Lamp Feed (Export) | E1 | RED | 122 | Rear Fog Lamp Feed (Export)
E2 | TAN | 159 | Key In Ignition Reminder Output | E2 | TAN | 159 | Key In Ignition Reminder Output
E3 | DK BLU | 49 | Driver Door Ajar Switch Signal | E3 | DK BLU | 49 | Driver Door Ajar Switch Signal
E4-E6 | -- | -- | Not Used | E4-E6 | -- | -- | Not Used
E7 | BLK/WHT | 238 | Seat Belt Switch Input | E7 | BLK/WHT | 238 | Seat Belt Switch Input
E8-E9 | -- | -- | Not Used | E8-E9 | -- | -- | Not Used
F1 | TAN | 294 | Passenger Door Lock Motor Feed-Unlock | F1 | TAN | 294 | Passenger Door Lock Motor Feed-Unlock
F2 | GRY | 295 | Passenger Door Lock Motor Feed-Lock | F2 | GRY | 295 | Passenger Door Lock Motor Feed-Lock
F3 | ORN | 54 | Door Jamb Switch Signal-Passenger | F3 | ORN | 54 | Door Jamb Switch Signal-Passenger
F4 | -- | -- | Not Used | F4 | -- | -- | Not Used
F6 | ORN | 2540 | Fused Battery Feed | F6 | ORN | 2540 | Fused Battery Feed
F7 | PPL | 293 | Rear Defogger Element Feed | F7 | PPL | 293 | Rear Defogger Element Feed
F8-G1 | -- | -- | Not Used | F8-G1 | -- | -- | Not Used
G2 | LT BLU | 195 | Door Lock Switch Input-Battery | G2 | LT BLU | 195 | Door Lock Switch Input-Battery
G3 | RED/BLK | 780 | Driver Door Lock-Key Cylinder | G3 | RED/BLK | 780 | Driver Door Lock-Key Cylinder
G4 | ORN/BLK | 781 | Driver Door Unlock-Key Cylinder | G4 | ORN/BLK | 781 | Driver Door Unlock-Key Cylinder
G5 | -- | -- | Not Used | G5 | -- | -- | Not Used
G6 | TAN | 694 | Driver Door Unlock-Motor Feed | G6 | TAN | 694 | Driver Door Unlock-Motor Feed
G7 | WHT | 194 | Door Unlock Switch Input-Battery | G7 | WHT | 194 | Door Unlock Switch Input-Battery
G8 | -- | -- | Not Used | G8 | -- | -- | Not Used
G9 | PPL | 709 | Left Park Lamp Feed | G9 | PPL | 709 | Left Park Lamp Feed
G10 | BRN/WHT | 309 | Right Park Lamp Feed | G10 | BRN/WHT | 309 | Right Park Lamp Feed

#### In-line Connector C201

Connector Part Information |

• | 12047842

• | 17-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | -- | -- | Not Used | A1 | -- | -- | Not Used
A2 | PNK | 539 | Fused Ignition 1 Feed | A2 | PNK | 539 | Fused Ignition 1 Feed
A3 | -- | -- | Not Used | A3 | -- | -- | Not Used
A4 | PPL | 16 | Turn Signal Flasher Output | A4 | PPL | 16 | Turn Signal Flasher Output
A5 | -- | -- | Not Used | A5 | -- | -- | Not Used
A6 | DK BLU | 15 | Turn Signal Lamp Feed-Right Front | A6 | DK BLU | 15 | Turn Signal Lamp Feed-Right Front
A7 | LT BLU | 14 | Turn Signal Lamp Feed-Left Front | A7 | LT BLU | 14 | Turn Signal Lamp Feed-Left Front
A8-A10 | -- | -- | Not Used | A8-A10 | -- | -- | Not Used
A11 | BLK | 28 | Horn Relay Output-Coil | A11 | BLK | 28 | Horn Relay Output-Coil
A12 | GRY | 397 | Cruise ON/OFF Signal | A12 | GRY | 397 | Cruise ON/OFF Signal
A13 | PNK | 739 | Fused Ignition 1 Feed | A13 | PNK | 739 | Fused Ignition 1 Feed
A14 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal | A14 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal
A15 | GRY/BLK | 87 | Cruise Control RESUME/ACCELERATE Switch Signal | A15 | GRY/BLK | 87 | Cruise Control RESUME/ACCELERATE Switch Signal
A16 | BLK | 434 | PARK/NEUTRAL Input | A16 | ORN/BLK | 434 | PARK/NEUTRAL Input
A17 | DK GRN/WHT | 1135 | Stop Lamp Switched BTSI Feed | A17 | DK GRN/WHT | 1135 | Stop Lamp Switched BTSI Feed

#### In-line Connector C201

Connector Part Information |

• | 12084183

• | 18-Way F Metri-Pack Mixed Series (BLK)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | BLK | 150 | Ground | B2 | BLK | 150 | Ground
B3 | LT GRN | 80 | Key In Ignition Input | B3 | LT GRN | 80 | Key In Ignition Input
B4 | TAN | 159 | Ground | B4 | BLK | 1550 | Ground
B5-B6 | -- | -- | Not Used | B5-B6 | -- | -- | Not Used
C1 | WHT | 1390 | Ignition Switched Battery Feed-Ignition 0 | C1 | WHT | 1390 | Ignition Switched Battery Feed-Ignition 0
C2 | BLK | 150 | Ground | C2 | BLK | 150 | Ground
C3-C4 | -- | -- | Not Used | C3C4 | -- | -- | Not Used
C5 | PNK | 3 | Ignition Switched Battery Feed-Ignition 1 | C5 | PNK | 3 | Ignition Switched Battery Feed-Ignition 1
C6 | ORN | 300 | Ignition Switched Battery Feed-Ignition 3 | C6 | ORN | 300 | Ignition Switched Battery Feed-Ignition 3
D1 | YEL | 5 | Ignition Switched Battery Feed-Crank | D1 | YEL | 5 | Ignition Switched Battery Feed-Crank
D2 | RED | 142 | Fused Battery Feed | D2 | RED | 142 | Fused Battery Feed
D3-D4 | -- | -- | Not Used | D3-D4 | -- | -- | Not Used
D5 | RED | 42 | Fused Battery Feed | D5 | RED | 42 | Fused Battery Feed
D6 | BRN | 4 | Ignition Switched Battery Feed-Accessory | D6 | BRN | 4 | Ignition Switched Battery Feed-Accessory

#### In-line Connector C201

Connector Part Information |

• | 12047840

• | 13-Way F Metri-Pack 280 Series (LT-GRY)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
E1 | LT BLU | 1508 | Turn Signal Lamp/Hazard Lamp Flasher Feed | E1 | LT BLU | 1508 | Turn Signal Lamp/Hazard Lamp Flasher Feed
E2 | DK GRN | 113 | Windshield Wiper Switch Signal-ON | E2 | DK GRN | 113 | Windshield Wiper Switch Signal-ON
E3 | GRY | 112 | Windshield Wiper Switch Signal-LOW/PULSE | E3 | GRY | 112 | Windshield Wiper Switch Signal-LOW/PULSE
E4 | PPL | 92 | Windshield Wiper Motor Feed-High Speed | E4 | PPL | 92 | Windshield Wiper Motor Feed-High Speed
E5 | RED | 228 | Windshield Washer Pump Motor Feed | E5 | RED | 228 | Windshield Washer Pump Motor Feed
E6 | DK GRN | 19 | Tail/Turn Stop Lamp Feed-Right Rear | E6 | DK GRN | 19 | Tail/Turn Stop Lamp Feed-Right Rear
E7 | YEL | 18 | Tail/Turn Stop Lamp Feed-Left Rear | E7 | YEL | 18 | Tail/Turn Stop Lamp Feed-Left Rear
E8 | ORN | 1840 | Fused Battery Feed | E8 | ORN | 1840 | Fused Battery Feed
E9 | YEL | 243 | Fused Accessory Feed | E9 | YEL | 243 | Fused Accessory Feed
E10 | YEL | 307 | Headlamp Switch Ouput-Flash to Pass | E10 | YEL | 307 | Headlamp Switch Ouput-Flash to Pass
E11 | LT GRN | 11 | High Beam Headlamp Feed | E11 | LT GRN | 11 | High Beam Headlamp Feed
E12 | TAN | 12 | Low Beam Headlamp Feed | E12 | TAN | 12 | Low Beam Headlamp Feed
E13 | YEL | 10 | Headlamp Switch Output | E13 | YEL | 10 | Headlamp Switch Output

#### In-line Connector C203

Connector Part Information |

• | 12034257

• | 56-Way F Metri-Pack Mixed Series (BLK)

Connector Part Information

• | 12186339

• | 56-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | ORN | 1052 | Auxiliary Blower Motor Output | A1 | ORN | 1052 | Auxiliary Blower Motor Output
A2 | YEL | 18 | Tail/Turn/Stop Lamp Feed-Left Rear | A2 | YEL | 18 | Tail/Turn/Stop Lamp Feed-Left Rear
A3 | DK GRN | 19 | Tail/Turn/Stop Lamp Feed-Right Rear | A3 | DK GRN | 19 | Tail/Turn/Stop Lamp Feed-Right Rear
A4 | LT BLU | 1134 | Park Brake Switch Signal (Domestic) | A4 | LT BLU | 1134 | Park Brake Switch Signal (Domestic)
A4 | TAN/WHT | 33 | Brake Warning Indicator Lamp Output (Export) | A4 | TAN/WHT | 33 | Brake Warning Indicator Lamp Output (Export)
A6 | -- | -- | Not Used | A6 | -- | -- | Not Used
A7 | GRY | 778 | Auxiliary Blower Motor Switch Output | A7 | GRY | 778 | Auxiliary Blower Motor Switch Output
A8 | WHT | 17 | Stop Lamp Switch Output | A8 | WHT | 17 | Stop Lamp Switch Output
A9 | BRN | 241 | Fused Ignition 3 Feed | A9 | BRN | 241 | Fused Ignition 3 Feed
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | GRY | 391 | Rear Window Wiper Switch Output | B2 | GRY | 391 | Rear Window Wiper Switch Output
B3 | BRN | 882 | RR Wheel Speed Signal-High | B3 | BRN | 882 | RR Wheel Speed Signal-High
B4 | WHT | 883 | RR Wheel Speed Signal-Low | B4 | WHT | 883 | RR Wheel Speed Signal-Low
B6 | BRN | 9 | Park Lamp Feed | B6 | BRN | 9 | Park Lamp Feed
B7 | WHT | 393 | Rear Window Wiper Motor Feed | B7 | WHT | 393 | Rear Window Wiper Motor Feed
B8 | DK GRN | 392 | Rear Window Washer Pump Motor Feed | B8 | DK GRN | 392 | Rear Window Washer Pump Motor Feed
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
C1 | BLK | 884 | LR Wheel Speed Signal-High | C1 | BLK | 884 | LR Wheel Speed Signal-High
C2 | RED | 885 | LR Wheel Speed Signal-Low | C2 | RED | 885 | LR Wheel Speed Signal-Low
C3 | LT BLU | 733 | Temperature Valve Position Signal | C3 | LT BLU | 733 | Temperature Valve Position Signal
C4 | GRY | 2700 | Fuel Tank Pressure Sensor 5 Volt Reference | C4 | GRY | 2700 | Fuel Tank Pressure Sensor 5 Volt Reference
C6 | YEL | 804 | Door Ajar Indicator Lamp Output | C6 | YEL | 804 | Door Ajar Indicator Lamp Output
C7 | DK BLU | 1128 | Class 2 Serial Data Communication | C7 | DK BLU | 1128 | Class 2 Serial Data Communication
C8 | PPL | 1589 | Fuel Gauge Sensor Input | C8 | PPL | 1589 | Fuel Gauge Sensor Input
C9 | YEL | 1127 | Class 2 Serial Data Line | C9 | YEL | 1127 | Class 2 Serial Data Line
D1 | LT BLU | 1072 | Auxiliary Blower Resistor Output-Medium | D1 | LT BLU | 1072 | Auxiliary Blower Resistor Output-Medium
D2 | BLK/WHT | 351 | Ground-Clean (Domestic) | D2 | BLK/WHT | 351 | Ground-Clean (Domestic)
D3 | GRY | 8 | Interior Lamp Dim Signal | D3 | GRY | 8 | Interior Lamp Dim Signal
D6 | PPL | 493 | Rear Seat Audio Enable Signal | D6 | PPL | 493 | Rear Seat Audio Enable Signal
D7 | BLK | 2759 | Fuel Tank Sensor Ground | D7 | BLK | 2759 | Fuel Tank Sensor Ground
D8 | ORN | 640 | Fused Battery Feed | D8 | ORN | 640 | Fused Battery Feed
E1 | DK BLU | 46 | Speaker Feed-Right Rear | E1 | DK BLU | 46 | Speaker Feed-Right Rear
E2 | TAN | 201 | Speaker Feed-Left Front | E2 | TAN | 201 | Speaker Feed-Left Front
E3 | LT GRN | 200 | Speaker Feed-Right Front | E3 | LT GRN | 200 | Speaker Feed-Right Front
E4 | YEL | 116 | Speaker Return-Left Rear | E4 | YEL | 116 | Speaker Return-Left Rear
E6 | LT BLU/BLK | 1505 | Heated Seat Switch Signal-Passenger | E6 | LT BLU/BLK | 1505 | Heated Seat Switch Signal-Passenger
E7 | LT BLU | 1462 | Heated Seat Switch Signal | E7 | LT BLU | 1462 | Heated Seat Switch Signal
E8 | LT GRN | 1011 | Remote Radio Control Signal (Domestic) | E8 | LT GRN | 1011 | Remote Radio Control Signal (Domestic)
E9 | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | E9 | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
F1 | GRY/BLK | 308 | Park Lamp Switch Output-Parklamps ON | F1 | GRY/BLK | 308 | Park Lamp Switch Output-Parklamps ON
F2-F4 | -- | -- | Not Used | F2-F4 | -- | -- | Not Used
F6 | YEL | 1176 | Auxiliary Blower Resistor Output-Low | F6 | YEL | 1176 | Auxiliary Blower Resistor Output-Low
F7 | LT GRN/BLK | 24 | Backup Lamp Feed (Domestic) | F7 | LT GRN | 24 | Backup Lamp Feed (Domestic)
F7 | LT GRN/BLK | 924 | Backup Lamp Feed (Export) | F7 | LT GRN | 924 | Backup Lamp Feed (Export)
F8 | BLK | 1550 | Ground | F8 | BLK | 1550 | Ground
F9 | PNK | 314 | Radio Signal-On (Domestic) | F9 | PNK | 314 | Radio Signal-On (Domestic)
G1 | -- | -- | Not Used | G1 | -- | -- | Not Used
G2 | BRN | 641 | Fused Ignition 3 Feed | G2 | BRN | 641 | Fused Ignition 3 Feed
G3 | PNK | 39 | Fused Ignition 1 Feed | G3 | PNK | 39 | Fused Ignition 1 Feed
G4 | WHT | 1310 | Canister Vent Valve Solenoid Output | G4 | WHT | 1310 | Canister Vent Valve Solenoid Output
G5 | PNK/BLK | 1303 | Liftgate Ajar Switch Signal | G5 | PNK/BLK | 1303 | Liftgate Ajar Switch Signal
G6 | -- | -- | Not Used | G6 | -- | -- | Not Used
G7 | BRN | 199 | Speaker Feed-Left Rear | G7 | BRN | 199 | Speaker Feed-Left Rear
G8 | LT BLU | 115 | Speaker Return-Right Rear | G8 | LT BLU | 115 | Speaker Return-Right Rear
G9 | DK GRN | 117 | Speaker Return-Right Front | G9 | DK GRN | 117 | Speaker Return-Right Front
G10 | GRY | 118 | Speaker Return-Left Front | G10 | GRY | 118 | Speaker Return-Left Front

#### In-line Connector C205

Connector Part Information |

• | 12092162

• | 4-Way F Metri-Pack 280 Series Sealed (GRY)

Connector Part Information

• | 12162477

• | 4-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 443 | Fused Accessory Feed | A | YEL | 443 | Fused Accessory Feed
B | GRY | 1244 | Fused I/P Dim Signal | B | BRN | 1244 | Fused I/P Dim Signal
C | LT GRN | 1796 | Radio Control Signal-Steering Column | C | DK BLU | 1796 | Radio Control Signal-Steering Column
D | BLK | 1450 | Ground | D | BLK | 1450 | Ground

#### In-line Connector C215

Connector Part Information |

• | 12092865

• | 2-Way F Metri-Pack 280 Series (YEL)

Connector Part Information

• | 12077934

• | 2-Way M Metri-Pack 280 Series (YEL)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 347 | SIR Inflator Feed-Driver | A | WHT | 347 | SIR Inflator Feed-Driver
B | DK GRN | 348 | SIR Inflator Output-Driver | B | DK GRN | 348 | SIR Inflator Output-Driver

#### In-line Connector C216

Connector Part Information |

• | 12110505

• | 2-Way F Metri-Pack 150 Series (YEL)

Connector Part Information

• | 12110288

• | 2-Way M Metri-Pack 280 Series (YEL)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK GRN/WHT | 1404 | Passenger Inflator Output-High | A | DK GRN/WHT | 1404 | Passenger Inflator Output-High
B | WHT/BLK | 1403 | Passenger Inflator Output-Low | B | WHT/BLK | 1403 | Passenger Inflator Output-Low

#### In-line Connector C301

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 194 | Door Unlock Switch Input-Battery | A | WHT | 194 | Door Unlock Switch Input-Battery
B | TAN | 294 | Driver Door Unlock-Battery | B | TAN | 294 | Driver Door Unlock-Battery
C | LT BLU | 195 | Door Lock Switch Input-Battery | C | LT BLU | 195 | Door Lock Switch Input-Battery
D | ORN | 267 | Heated Mirror Feed | D | ORN | 267 | Heated Mirror Feed
E-K | -- | -- | Not Used | E-K | -- | -- | Not Used

#### In-line Connector C302

Connector Part Information |

• | 12129430

• | 16-Way F ACT 280 Series (WHT)

Connector Part Information

• | 12129429

• | 16-Way M ACT 280 Series (WHT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 750 | Ground | A | BLK | 750 | Ground
B | DK GRN | 117 | Speaker Return-Right Front | B | DK GRN | 117 | Speaker Return-Right Front
C | LT GRN | 200 | Speaker Feed-Right Front | C | LT GRN | 200 | Speaker Feed-Right Front
D | -- | -- | Not Used | D | -- | -- | Not Used
E | YEL | 143 | Fused Accessory Feed | E | YEL | 143 | Fused Accessory Feed
F | LT BLU | 166 | LH Front Window Switch Feed-RH Front Window UP | F | LT BLU | 166 | LH Front Window Switch Feed-RH Front Window UP
G | DK BLU | 49 | Driver Door Ajar Switch Signal | G | DK BLU | 49 | Driver Door Ajar Switch Signal
H | YEL | 804 | Door Ajar Indicator Lamp Output | H | YEL | 804 | Door Ajar Indicator Lamp Output
J | GRY | 8 | Interior Lamp Dim Signal | J | GRY | 8 | Interior Lamp Dim Signal
K | TAN | 167 | LH Front Window Switch Feed-RH Front Window DOWN | K | TAN | 167 | LH Front Window Switch Feed-RH Front Window DOWN
L | RED/BLK | 780 | Door Lock-Key Cylinder | L | RED/BLK | 780 | Door Lock-Key Cylinder
M | ORN/BLK | 781 | Door Unlock-Key Cylinder | M | ORN/BLK | 781 | Door Unlock-Key Cylinder
N | RED/WHT | 881 | RH Outside Rearview Mirror Right/Left Feed | N | RED/WHT | 881 | RH Outside Rearview Mirror Right/Left Feed
P | LT BLU/WHT | 1497 | RH Outside Rearview Mirror Motor Pack Common Feed | P | LT BLU/WHT | 1497 | RH Outside Rearview Mirror Motor Pack Common Feed
R | BRN/WHT | 1498 | RH Outside Rearview Mirror UP/DOWN Feed | R | BRN/WHT | 1498 | RH Outside Rearview Mirror UP/DOWN Feed
S | GRY | 295 | Passenger Door Lock Motor Feed-Lock | S | GRY | 295 | Passenger Door Lock Motor Feed-Lock

#### In-line Connector C303

Connector Part Information |

• | 12129430

• | 16-Way F ACT 280 Series (WHT)

Connector Part Information

• | 12129429

• | 16-Way M ACT 280 Series (WHT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 750 | Ground | A | BLK | 750 | Ground
B | GRY | 118 | Speaker Return-Left Front | B | GRY | 118 | Speaker Return-Left Front
C | TAN | 201 | Speaker Feed-Left Front | C | TAN | 201 | Speaker Feed-Left Front
D | ORN | 1140 | Fused Battery Feed | D | ORN | 1140 | Fused Battery Feed
E | YEL | 143 | Fused Ignition 3 Feed | E | YEL | 143 | Fused Ignition 3 Feed
F | LT BLU | 166 | LH Front Window Switch Feed-RH Front Window UP | F | LT BLU | 166 | LH Front Window Switch Feed-RH Front Window UP
G | TAN | 159 | Key In Ignition Output | G | TAN | 159 | Key In Ignition Output
H | YEL | 804 | Door Ajar Indicator Lamp Output | H | YEL | 804 | Door Ajar Indicator Lamp Output
J | GRY | 8 | Interior Lamp Dim Signal | J | GRY | 8 | Interior Lamp Dim Signal
K | TAN | 167 | LH Front Window Switch Feed-RH Front Window DOWN | K | TAN | 167 | LH Front Window Switch Feed-RH Front Window DOWN
L | RED/BLK | 780 | Door Lock-Key Cylinder | L | RED/BLK | 780 | Door Lock-Key Cylinder
M | ORN/BLK | 781 | Door Unlock-Key Cylinder | M | ORN/BLK | 781 | Door Unlock-Key Cylinder
N | RED/WHT | 881 | RH Outside Rearview Mirror Right/Left Feed | N | RED/WHT | 881 | RH Outside Rearview Mirror Right/Left Feed
P | LT BLU/WHT | 1497 | RH Outside Rearview Mirror Motor Pack Common Feed | P | LT BLU/WHT | 1497 | RH Outside Rearview Mirror Motor Pack Common Feed
R | BRN/WHT | 1498 | RH Outside Rearview Mirror UP/DOWN Feed | R | BRN/WHT | 1498 | RH Outside Rearview Mirror UP/DOWN Feed
S | GRY | 295 | Passenger Door Lock Motor Feed-Lock | S | GRY | 295 | Passenger Door Lock Motor Feed-Lock

#### In-line Connector C304

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 194 | Door Unlock Switch Input-Battery | A | WHT | 194 | Door Unlock Switch Input-Battery
B | TAN | 294 | Passenger Door Lock Motor Feed-Unlock | B | TAN | 294 | Passenger Door Lock Motor Feed-Unlock
C | LT BLU | 195 | Door Lock Switch Input-Battery | C | LT BLU | 195 | Door Lock Switch Input-Battery
D | ORN | 267 | Heated Mirror Feed | D | ORN | 267 | Heated Mirror Feed
E-K | -- | -- | Not Used | E-K | -- | -- | Not Used

#### In-line Connector C305

Connector Part Information |

• | 12146439

• | 4-Way F Metri-Pack 150 Series Sealed (GRY)

Connector Part Information

• | 15326714

• | 12-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
2A | BRN | 882 | RR Wheel Speed Signal-High | 1A | BRN | 882 | RR Wheel Speed Signal-High
2B | WHT | 883 | RR Wheel Speed Signal-Low | 1B | WHT | 883 | RR Wheel Speed Signal-Low
2C | BLK | 884 | LR Wheel Speed Signal-High | 1C | BLK | 884 | LR Wheel Speed Signal-High
2D | RED | 885 | LR Wheel Speed Signal-Low | 1D | RED | 885 | LR Wheel Speed Signal-Low

#### In-line Connector C305

Connector Part Information |

• | 12176335

• | 8-Way F Metri Pack 280 Flexlock Series Sealed (NAT)

Connector Part Information

• | 15326714

• | 12-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 250 | Ground | 3A | BLK | 250 | Ground
B | BLK | 2759 | Fuel Level Gauge Sensor Signal | 3B | BLK | 2759 | Fuel Level Gauge Sensor Signal
C | GRY | 120 | Fuel Pump Motor Feed | 3C | GRY | 120 | Fuel Pump Motor Feed
D | PPL | 1589 | Fuel Gauge Sensor Signal | 3D | PPL | 1589 | Fuel Gauge Sensor Signal
E | DK GRN | 890 | Fuel Gauge Sensor Signal | 3E | DK GRN | 890 | Fuel Gauge Sensor Signal
F | WHT | 1310 | Canister Vent Valve Solenoid Output | 3F | WHT | 1310 | Canister Vent Valve Solenoid Output
G | PNK | 1039 | Fused Ignition 1 Feed | 3G | PNK | 1039 | Fused Ignition 1 Feed
H | GRY | 2700 | 5 Volt Reference | 3H | GRY | 2700 | 5 Volt Reference

#### In-line Connector C306

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12162000 (SWB)

• | 12186216 (LWB)

• | 2-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 882 | RR Wheel Speed Signal-High | A | BRN | 882 | RR Wheel Speed Signal-High
B | WHT | 883 | RR Wheel Speed Signal-Low | B | WHT | 883 | RR Wheel Speed Signal-Low

#### In-line Connector C308

Connector Part Information |

• | 12092249

• | 23-Way F ACT 280 Series (BLK)

Connector Part Information

• | 12092248

• | 23-Way M ACT 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 901 | Rear Quarter Window Switch-Close | A | BLK | 901 | Rear Quarter Window Switch-Close
B | LT GRN/BLK | 735 | Ambient Air Temperature Sensor Signal | B | LT GRN/BLK | 735 | Ambient Air Temperature Sensor Signal
C-D | -- | -- | Not Used | C-D | -- | -- | Not Used
E | BLK/WHT | 1896 | Power Sliding Door System Switch Signal | E | BLK/WHT | 1896 | Power Sliding Door System Switch Signal
F | YEL | 1127 | Class 2 Serial Data Communication | F | YEL | 1127 | Class 2 Serial Data Communication
G | GRY | 8 | Interior Lamp Dim Signal | G | GRY | 8 | Interior Lamp Dim Signal
H | BRN | 241 | Fused Ignition 3 Feed | H | BRN | 241 | Fused Ignition 3 Feed
J | BLK | 1550 | Ground | J | BLK | 1550 | Ground
K | YEL | 743 | Fused Accessory Feed | K | YEL | 743 | Fused Accessory Feed
L | -- | -- | Not Used | L | -- | -- | Not Used
M | GRY/BLK | 308 | Park Lamp Switch Output-Parklamps ON | M | GRY/BLK | 308 | Park Lamp Switch Output-Parklamps ON
N | ORN | 640 | Fused Battery Feed | N | ORN | 640 | Fused Battery Feed
P-R | -- | -- | Not Used | P-R | -- | -- | Not Used
S | GRY/BLK | 690 | Courtesy Lamp Control | S | GRY/BLK | 690 | Courtesy Lamp Control
T | -- | -- | Not Used | T | -- | -- | Not Used
U | LT BLU | 1894 | Power Sliding Door Switch Signal | U | LT BLU | 1894 | Power Sliding Door Switch Signal
V | -- | -- | Not Used | V | -- | -- | Not Used
W | DK BLU | 1393 | Courtesy Lamps Feed-Protected Battery | W | DK BLU | 1393 | Courtesy Lamps Feed-Protected Battery
X | PPL | 328 | Interior Lamp Override Switch Output | X | PPL | 328 | Interior Lamp Override Switch Output
Y | -- | -- | Not Used | Y | -- | -- | Not Used
Z | BRN | 902 | Rear Quarter Window Switch-Open | Z | BRN | 902 | Rear Quarter Window Switch-Open

#### In-line Connector C309

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12162000 (SWB)

• | 12186216 (LWB)

• | 2-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 884 | LR Wheel Speed Signal-High | A | BLK | 884 | LR Wheel Speed Signal-High
B | WHT | 885 | LR Wheel Speed Sensor-Low | B | RED | 885 | LR Wheel Speed Sensor-Low

#### In-line Connector C313 / C314

Connector Part Information |

• | 12064749

• | 2-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12064750

• | 2-Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN/BLK | 340 | Fused Battery Feed | A | ORN | 340 | Fused Battery Feed
B | BLK | 550 | Ground | B | BLK | 550 | Ground

#### In-line Connector C315

Connector Part Information |

• | 12129136

• | 4-Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129135

• | 4-Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 340 | Battery Positive Voltage | A | YEL | -- | Battery Positive Voltage
B | LT BLU | 1462 | Heated Seat Switch Signal | B | LT BLU | -- | Heated Seat Switch Signal
C | BLK | 550 | Ground | C | BLK | -- | Ground
D | -- | -- | Not Used | D | -- | -- | Not Used

#### In-line Connector C316

Connector Part Information |

• | 12129136

• | 4-Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129135

• | 4-Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 340 | Battery Positive Voltage | A | YEL | -- | Battery Positive Voltage
B | LT BLU | 1505 | Heated Seat Switch Signal | B | LT BLU | -- | Heated Seat Switch Signal
C | BLK | 550 | Ground | C | BLK | -- | Ground
D | -- | -- | Not Used | D | -- | -- | Not Used

#### In-line Connector C400

Connector Part Information |

• | 12015199

• | 2-Way F Metri-Pack 280 Series (NAT)

Connector Part Information

• | 12015271

• | 2-Way M Metri-Pack 280 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 450 | Ground | A | BLK | 450 | Ground
B | PPL | 293 | Rear Defogger Element Feed | B | PPL | 293 | Rear Defogger Element Feed

#### In-line Connector C401

Connector Part Information |

• | 12047785

• | 4-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047786

• | 4-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED/BLK | 780 | Door Lock-Key Cylinder | A | RED/BLK | 780 | Door Lock-Key Cylinder
B | ORN/BLK | 781 | Door Unlock-Key Cylinder | B | ORN/BLK | 781 | Door Unlock-Key Cylinder
C | GRY | 391 | Rear Window Wiper Switch Output | C | GRY | 391 | Rear Window Wiper Switch Output
D | DK GRN | 392 | Rear Window Washer Pump Motor Feed | D | DK GRN | 392 | Rear Window Washer Pump Motor Feed

#### In-line Connector C402

Connector Part Information |

• | 12047886

• | 8-Way F Metri-Pack 150 Flexlock Series Sealed (BLK)

Connector Part Information

• | 12045688

• | 8-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 116 | Speaker Return-Left Rear | A | YEL | 116 | Speaker Return-Left Rear
B | BRN | 199 | Speaker Feed-Left Rear | B | BRN | 199 | Speaker Feed-Left Rear
C | BRN | 9 | Park Lamp Feed | C | BRN | 9 | Park Lamp Feed
D | WHT | 17 | Stop Lamp Switch Output | D | WHT | 17 | Stop Lamp Switch Output
E | PNK/BLK | 1303 | Liftgate Ajar Indicator Lamp Output | E | PNK/BLK | 1303 | Liftgate Ajar Indicator Lamp Output
F | DK BLU | 49 | Driver Door Ajar Switch Signal | F | DK BLU | 49 | Driver Door Ajar Switch Signal
G | DK BLU | 46 | Speaker Feed-Right Rear | G | DK BLU | 46 | Speaker Feed-Right Rear
H | LT BLU | 115 | Speaker Return-Right Rear | H | LT BLU | 115 | Speaker Return-Right Rear

#### In-line Connector C403

Connector Part Information |

• | 12020397

• | 3-Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12020398

• | 3-Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TAN | 294 | Passenger Door Lock Motor Feed-Unlock | A | TAN | 294 | Passenger Door Lock Motor Feed-Unlock
B | GRY | 295 | Passenger Door Lock Motor Feed-Lock | B | GRY | 295 | Passenger Door Lock Motor Feed-Lock
C | WHT | 393 | Rear Window Wiper Motor Feed | C | WHT | 393 | Rear Window Wiper Motor Feed

#### In-line Connector C405

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1240 | Fused Battery Feed | A | ORN | 1240 | Fused Battery Feed
B | RED | 122 | Rear Fog Lamp Feed (Export) | B | RED | 122 | Rear Fog Lamp Feed (Export)
C | DK GRN | 19 | Tail/Turn/Stop Lamp Feed-Right Rear | C | DK GRN | 19 | Tail/Turn/Stop Lamp Feed-Right Rear
D | YEL | 18 | Tail/Turn/Stop Lamp Feed-Left Rear | D | YEL | 18 | Tail/Turn/Stop Lamp Feed-Left Rear
E | YEL | 743 | Fused Accessory Feed | E | YEL | 743 | Fused Accessory Feed
F | WHT | 17 | Stop Lamp Switch Output | F | WHT | 17 | Stop Lamp Switch Output
G | BRN | 9 | Park Lamp Feed (Domestic) | G | BRN | 9 | Park Lamp Feed (Domestic)
G | PPL | 709 | Left Park Lamp Feed (Export) | G | PPL | 709 | Left Park Lamp Feed (Export)
H | BLK | 1725 | Ground | H | BLK | 1725 | Ground
J | BRN/WHT | 309 | Right Park Lamp Feed | J | BRN/WHT | 309 | Right Park Lamp Feed
K | -- | -- | Not Used | K | -- | -- | Not Used

#### In-line Connector C407 (Domestic)

Connector Part Information |

• | 12052848

• | 6-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12124107

• | 6-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1240 | Fused Battery Feed | A | ORN | 1240 | Fused Battery Feed
B | BRN | 9 | Park Lamp Feed | B | BRN | 9 | Park Lamp Feed
C | YEL | 18 | Tail/Turn/Stop Lamp Feed-Left Rear | C | YEL | 18 | Tail/Turn/Stop Lamp Feed-Left Rear
D | DK GRN | 19 | Tail/Turn/Stop Lamp Feed-Right Rear | D | DK GRN | 19 | Tail/Turn/Stop Lamp Feed-Right Rear
E | WHT | 17 | Stop Lamp Switch Output | E | WHT | 17 | Stop Lamp Switch Output
F | BLK | 1725 | Ground | F | BLK | 1725 | Ground

#### In-line Connector C407 (Export)

Connector Part Information |

• | 12047937

• | 8-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047931

• | 8-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | ORN | 1240 | Fused Battery Feed | A | ORN | 1240 | Fused Battery Feed
B | RED | 122 | Rear Fog Lamp Feed | B | RED | 122 | Rear Fog Lamp Feed
C | YEL | 18 | Tail/Turn/Stop Lamp Feed-Left Rear | C | YEL | 18 | Tail/Turn/Stop Lamp Feed-Left Rear
D | DK GRN | 19 | Tail/Turn/Stop Lamp Feed-Right Rear | D | DK GRN | 19 | Tail/Turn/Stop Lamp Feed-Right Rear
E | WHT | 17 | Stop Lamp Switch Output | E | WHT | 17 | Stop Lamp Switch Output
F | BLK | 1725 | Ground | F | BLK | 1725 | Ground
G | PPL | 709 | Left Park Lamp Feed | G | PPL | 709 | Left Park Lamp Feed
H | BRN/WHT | 309 | Right Park Lamp Feed | H | BRN/WHT | 309 | Right Park Lamp Feed