For 1990-2009 cars

1. Inspect the wiring harness assembly (224) for:

• | Cut or pinched wires

• | Cut wire insulation

• | Bent or broken electrical connectors

• | Damaged terminal pins

2. Position the wire harness assembly (224) onto the control valve body (300) and the pump cover (201).
3. Mate each connector into its respective electrical component and engage the locking tabs.
4. Secure the wiring harness conduit into the retaining clip (226) on the pump cover (201).
5. Assemble the fluid temperature sensor (391) into the temperature sensor clip (390).