For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Bucket Seat Replacement .
2. Turn the front seat upside down on a clean, flat surface.
3. Reach under and unfasten the front seat cushion support from the bottom of the front seat cushion frame.
4. Remove the cushion support from the front seat.

### Installation Procedure

1. Install the cushion support to the front seat.
2. Reach under and fasten the front seat cushion support to the bottom of the front seat cushion frame.
3. Install the front seat. Refer to Bucket Seat Replacement .