For 1990-2009 cars

Table 1: | Liftgate Door Lock Connector C1 (Ajar Indicator Switch)
Table 2: | Liftgate Door Lock Connector C2 (Actuator)
Table 3: | Liftgate Door Lock Cylinder Switch

#### Liftgate Door Lock Connector C1 (Ajar Indicator Switch)

Connector Part Information |

• | 1216-2190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 49 | Passenger Door Ajar Switch Signal
B | YEL | 9804 | Liftgate Ajar Indicator Lamp Output
C | -- | -- | Not Used
D | BLK | 450 | Ground

#### Liftgate Door Lock Connector C2 (Actuator)

Connector Part Information |

• | 1530-0027

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 294 | Passenger Door Unlock Input
B | GRY | 295 | Passenger Door Lock Input

#### Liftgate Door Lock Cylinder Switch

Connector Part Information |

• | 1211-0293

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/BLK | 780 | Door Lock-Key Cylinder Output to BCM
B | ORN/BLK | 781 | Door Unlock-Key Cylinder Output to BCM
C | BLK | 450 | Ground