For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views | Body Control System Connector End Views
Data Link Connector | Below the steering column, on the bottom of the knee bolster. | Data Link Communications Component Views | Data Link Communications Connector End Views
Liftgate Door Lock (Ajar Indicator Switch) | Part of the liftgate door lock | Body Rear End Component Views | Body Rear End Connector End Views
Pass Key III Module | In the steering column, at the ignition switch | -- | Theft Deterrent System Connector End Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Remote Control Door Lock Receiver (RCDLR) | Behind the center of the IP, underside of the IP trim, near the windshield defrost vent | Keyless Entry Component Views | Keyless Entry Connector End Views
Security Indicator Lamp | Center of the IP, mounted to the trim plate, near the windshield defrost vent | Theft Deterrent System Component Views | --
Theft Deterrent Shock Sensor | Below the left side IP, right of the steering column | Theft Deterrent System Component Views | Theft Deterrent System Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
C101 (20 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, near the EBCM | Harness Routing Views | Inline Harness Connector End Views
C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | -- | Inline Harness Connector End Views
C402 (8 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | -- | Inline Harness Connector End Views
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views | --
S202 | IP harness, leftt side of the IP approximately 15 cm (6 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S210 | IP harness, center of the IP approximately 4 cm (2 in) from the security indicator lamp breakout | -- | --
S211 | IP harness, left side of the IP approximately 15 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the liftgate lock cylinder switch breakout | -- | --