For 1990-2009 cars

### Removal Procedure

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gages and Console.
3. Slide the daytime running lamp module from the bracket.
4. Disconnect the electrical connectors.

### Installation Procedure

1. Position the daytime running lamp module in the bracket.
2. Slide the daytime running lamp module into the bracket in order to secure the module.
3. Connect the electrical connectors.
4. Install the instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gages and Console.
5. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.