For 1990-2009 cars

#### Tools Required

• | J 3289-20 Holding Fixture Base

• | J 28664-B Transmission Holding Fixture

• | J 44465 Holding Fixture Adapter (if required)

1. Install J 44465 onto J 28664-B (if required).
2. Install J 28664-B onto the transmission.
3. Install the transmission and holding fixture into J 3289-20 .
4. Insert the pin into J 3289-20 in order to hold the transmission in the desired position.