For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Ground (Negative) Cable Nut to Transaxle Stud | 25 N·m | 18 lb ft
Battery Ground (Negative) Cable to Inner Fender Bolt | 5 N·m | 44 lb in
Battery Hold-Down Retainer Bolt | 25 N·m | 18 lb ft
Battery Positive Cable to Underhood Electrical Center Nut | 10 N·m | 89 lb in
Battery Terminal Bolt | 16 N·m | 12 lb ft
Battery Tray Bolt | 10 N·m | 89 lb in
Generator B+ Terminal Nut | 13 N·m | 115 lb in
Generator Bolt | 50 N·m | 37 lb ft
Generator Bracket Bolt | 50 N·m | 37 lb ft
Generator Rear Cover Nut | 12 N·m | 106 lb in
Generator Rear Cover Screw | 4 N·m | 35 lb in
Generator Voltage Regulator Retaining Screw | 2 N·m | 18 lb in
Generator Voltage Regulator Terminal Screw | 1 N·m | 9 lb in
Spark Plug | 15 N·m | 11 lb ft
Starter Motor Bolt | 47 N·m | 35 lb ft
Starter Motor BAT Terminal Nut | 10 N·m | 89 lb in
Starter Motor S Terminal Nut | 3 N·m | 27 lb in