For 1990-2009 cars

Condition | Action
--- | ---
The power steering fluid level is low. | Fill the power steering system. Refer to Checking and Adding Power Steering Fluid .
The steering gear valve is sticking. |

1. Drain the power steering system. Refer to Draining the Power Steering System .
2. Fill the power steering system. Refer to Refilling the Power Steering System .
3. Bleed the power steering system. Refer to Power Steering System Bleeding .

Repair or replace the power steering gear if the symptoms persist. Refer to Steering Gear Replacement .

The power steering pump pressure is low. | Repair or replace the power steering pump. Refer to Power Steering Pump Replacement .