For 1990-2009 cars

1. Use a long screwdriver in order to depress the reverse band servo cover (40) by prying against the transmission holding fixture.
2. Use a small screwdriver in order to pry out the retaining ring (39) from the reverse band servo cover.
3. Remove the long screwdriver. The servo assembly will push the servo cover (40) up.
4. Remove the servo cover (40) and the servo cover O-ring seal (41).
5. Remove the reverse band servo assembly (42-48).
6. Remove the reverse band servo piston spring (49).