For 1990-2009 cars

### Removal Procedure

1. Open and support the hood.
2. Remove the primary hood latch. Refer to Hood Primary Latch Replacement .
3. Remove the bolts from the hood latch support at the upper tie bar.
4. Remove the hood latch support from the upper tie bar.

### Installation Procedure

1. Install the hood latch support to upper tie bar.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts to the hood latch support at the upper tie bar.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

3. Install the primary hood latch. Refer to Hood Primary Latch Replacement .
4. Close the hood.