For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Door Trim Panel Replacement in Doors.
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement in Doors.
3. Disconnect the electrical connector.
4. Unsnap the speaker from the lock module.

### Installation Procedure

1. Snap the speaker into the lock module.
2. Connect the electrical connector.
3. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement in Doors.
4. Install the front door trim panel. Refer to Door Trim Panel Replacement in Doors.