For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door locating pin screws.
2. Remove the sliding door locating pin from the vehicle.

### Installation Procedure

1. Install the sliding door locating pin to the sliding door.
2. Loosely install the sliding door locating pin screws, just tightly enough to retain the locating pin.
3. Close and then reopen the sliding door.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Re-torque the locating pin screws to the sliding door.

Tighten
Tighten the sliding door locating pin screws to 10 N·m (89 lb in).