For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

1. Remove the seat belt shoulder belt guide loop. Refer to Front Seat Shoulder Belt Guide Adjuster Replacement .
2. Remove the body pillar upper trim panel retainers using the J 38778 .
3. Remove the body pillar upper trim panel from the vehicle.

### Installation Procedure

1. Install the body pillar upper trim panel to the vehicle by aligning the locator tabs.
2. Align the body pillar upper trim panel retainers to the holes and pushing in on the retainers to secure them.
3. Install door opening seals to edge of body pillar upper trim panel.
4. Install the seat belt shoulder belt guide loop. Refer to Front Seat Shoulder Belt Guide Adjuster Replacement .