For 1990-2009 cars

## Exhaust Manifold Removal Right Side

1. Remove the heated oxygen sensor.
2. Remove the exhaust manifold heat shield bolts.
3. Remove the exhaust manifold heat shields.
4. Remove the right side spark plugs.
5. Remove the exhaust manifold nuts.
6. Remove the exhaust manifold.
7. Remove the exhaust manifold gasket.

## Exhaust Manifold Removal Left Side

1. Remove the exhaust manifold heat shield bolts.
2. Remove the exhaust manifold heat shield.
3. Remove the exhaust manifold nuts.
4. Remove the exhaust manifold.
5. Remove the exhaust manifold gasket.