For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat. Refer to Rear Seat Replacement .

Important: Each rear seat riser has a specific lock-out pin location, depending on the seat configuration. Note the location of the lock-out pins before removing, in order to properly reinstall the lock-out pins on the seat riser.

2. Remove the lock-out pins from the front legs of the seat riser.

### Installation Procedure

1. Install the lock-out pins to the front legs of the seat riser.
2. Install the rear seat. Refer to Rear Seat Replacement .