For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Heater-A/C Control (Rear Window Defogger Switch) | Part of the heater-A/C control | HVAC Component Views | HVAC Connector End Views
Outside Rearview Mirror | On the outside of the front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Outside Rearview Mirror (Heated Defogger) | In the outside rearview mirror | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Window Defogger Grid | Rear liftgate window | Stationary Windows Component Views | Stationary Windows Connector End Views
Relay Center | Right side of IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Power and Grounding Component Views | Power and Grounding Connector End Views
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views | Inline Harness Connector End Views
C301 (10 cavities) | Body wiring harness to the left side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views | Inline Harness Connector End Views
C302 (16 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views | Inline Harness Connector End Views
C303 (16 cavities) | Body wiring harness to the left front side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views | Inline Harness Connector End Views
C304 (10 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views | Inline Harness Connector End Views
C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | -- | Inline Harness Connector End Views
G401 | Secured to the lower left D-pillar | -- | --
P406 | Between the right side of the liftgate and the roof | Harness Routing Views | --
P500 | Between the left A-pillar and the left front door | Harness Routing Views | --
P600 | Between the right A-pillar and the right front door | Harness Routing Views | --
S213 | IP harness, center of IP approximately 72 cm (28 in) from the cigar lighter | -- | --
S264 | IP harness, right side of the IP approximately 16 cm (6 in) from the relay center breakout | -- | --
S275 | IP harness, right side of the IP approximately 6 cm (2.5 in) from the BCM breakout | -- | --
S303 | Body harness, front of the right B-pillar approximately 26 cm (10 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S318 | Body harness, under the right front door sill approximately 17 cm (7 in) C302 breakout | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the liftgate lock cylinder switch breakout | -- | --
S504 | Left door harness, left door approximately 10 cm (4 in) from the left window switch breakout | -- | --
S604 (w/ABS) | Right door harness, right door approximately 10 cm (4 in) from the right window switch breakout | -- | --
S604 (w/o ABS) | Right door harness, between P600 and the right front speaker breaker | -- | --