For 1990-2009 cars

#### Air Injection BL Value

Connector Part Information |

• | 12052641

• | 2 Way F Metric-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 339 | Fused Ignition Feed
B | PNK/BLK | 429 | Air Injection BL Valve Control

#### Automatic Transaxle (C111)

Connector Part Information |

• | 12160493

• | 20-Way F Metri-Packard 100 W Series Sealed (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 1222 | 1-2 shift solenoid valve control
B | YEL/BLK | 1223 | 2-3 shift solenoid valve control
C | RED/BLK | 1228 | Pressure control solenoid high
D | LT BLU/WHT | 1229 | Pressure control Solenoid low
E | PNK | 1339 | Fused ignition 1 feed
F-K | -- | -- | Not Used
L | YEL/BLK | 1227 | Transmission fluid temperature sensor signal
M | BLK | 2762 | Sensor ground
N | PNK | 1224 | Pressure switch A input
P | RED | 1226 | Pressure switch C input
R | DK BLU | 1225 | Pressure switch B input
S | RED/BLK | 1230 | Sensor ground
T | BRN | 418 | TCC PWM solenoid valve control
U | YEL | 657 | TCC Release switch input
V | DK BLU/WHT | 1231 | Sensor low
W | -- | -- | Not Used

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 12110293

• | 3-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/WHT | 812 | CMP sensor battery positive voltage (B+)
B | BLK | 630 | CMP sensor signal
C | BLK | 407 | CMP sensor ground

#### Crankshaft Position (CKP) Sensor (7X)

Connector Part Information |

• | 12162194

• | 2 Way F Metri-Pack 150 Series Seal (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 573 | 7X Reference High
B | PPL | 574 | 7X Reference Low

#### Camshaft Position (CKP) Sensor (24X)

Connector Part Information |

• | 12110293

• | 3 Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 1867 | CMP/CKP sensor ground
B | LT BLU/BLK | 647 | CKP sensor signal
C | YEL/BLK | 1868 | CMP/CKP sensor battery positive voltage

#### Engine Coolant Temp (ECT) Sensor

Connector Part Information |

• | 12162195

• | 2 Way

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | MAP Sensor Return
B | YEL | 410 | ECT Sensor Signal

#### Engine Oil Level Indicator Switch

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 1174 | Engine oil level indicator input
B | BLK/WHT | 451 | Ground

#### Engine Oil Pressure Indicator Switch

Connector Part Information |

• | 12065401

• | 1 Way F Metric-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/BLK | 231 | Oil Pressure Switch Signal
B | -- | -- | Not Used
C | -- | -- | Not Used
D | -- | -- | Not Used

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (Red)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 339 | Fused ignition 1 feed
B | DK GRN/WHT | 428 | EVAP canister purge valve control

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (Red)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 1039 | Fused ignition 1 feed
B | WHT | 1310 | Canister vent valve solenoid output

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | 15326389

• | 5-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 435 | EGR solenoid output
B | BLK | 2753 | PCM Sensor ground
C | BRN | 1456 | EGR solenoid position signal
D | GRY | 2702 | 5-volt reference A
E | RED | 1676 | EGR valve coil feed

#### Fuel Injector 1

Connector Part Information |

• | 15326179

• | 2 Way F Metric-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Fuse Output-IGN 1
B | BLK | 1744 | Fuel Injector 1 Output

#### Fuel Injector 2

Connector Part Information |

• | 15326179

• | 2 Way F Metric-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Fuse Output-IGN 1
B | LT GRN/BLK | 1745 | Fuel Injector 2 Output

#### Fuel Injector 3

Connector Part Information |

• | 15326179

• | 2 Way F Metric-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Fuse Output-IGN 1
B | PNK/BLK | 1746 | Fuel Injector 3 Output

#### Fuel Injector 4

Connector Part Information |

• | 15326179

• | 2 Way F Metric-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Fuse Output-IGN 1
B | LT BLU/BLK | 844 | Fuel Injector 4 Output

#### Fuel Injector 5

Connector Part Information |

• | 15326179

• | 2 Way F Metric-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Fuse Output-IGN 1
B | BLK/WHT | 845 | Fuel Injector 5 Output

#### Fuel Injector 6

Connector Part Information |

• | 15326179

• | 2 Way F Metric-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Fuse Output-IGN 1
B | YEL/BLK | 846 | Fuel Injector 6 Output

#### Fuel Pump Sender Unit C1

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 1589 | Fuel level sensor input
B | GRY | 120 | Fuel pump motor feed
C | BLK | 250 | Ground
D | BLK/WHT | 2759 | Ground-clean

#### Fuel Tank Pressure Sensor C2

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 2759 | Ground-clean
B | DK GRN | 890 | Fuel tank pressure sensor signal
C | GRY/BLK | 2700 | 5-volt reference

#### Heated Oxygen Sensor 1 (HO2S 1)

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 413 | HO2S 1 low
B | PPL | 412 | HO2S 1 signal
C | BLK | 1050 | Ground
D | PNK | 339 | Fused ignition 1 feed

#### Heated Oxygen Sensor 2 (HO2S 2)

Connector Part Information |

• | 12160825

• | 4-Way M Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1669 | HO2S 2 low
B | PPL/WHT | 1668 | HO2S 2 signal
C | BLK | 1050 | Ground
D | PNK | 339 | Fused ignition 1 feed

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 12162190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 444 | IAC motor feed-coil B low
B | LT GRN/WHT | 1749 | IAC motor feed-coil B high
C | LT BLU/BLK | 1748 | IAC motor feed-coil A low
D | LT BLU/WHT | 1747 | IAC motor feed-coil A high

#### Ignition Control Module (ICM) C1

Connector Part Information |

• | 12162260

• | 6-Way F Metri-Pack 150.2 Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/BLK | 424 | Electronic spark timing bypass signal
B | WHT | 423 | Electronic spark timing control signal
C-D | -- | -- | Not Used
E | PPL/WHT | 430 | Electronic spark timing high reference signal
F | RED/BLK | 453 | Electronic spark timing low reference signal

#### Ignition Control Module (ICM) C2

Connector Part Information |

• | 12162194

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 51 | Ground-clean
B | PNK | 239 | Fused ignition 1 feed

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 12162199

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2760 | IAT ground
B | TAN | 472 | IAT sensor input

#### Manifold Air Pressure (MAP) Sensor

Connector Part Information |

• | 12020403

• | 3 Way M Weather-Pack TRW Sealed (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | MAP Sensor Return
B | LT GRN | 432 | MAP Sensor Signal
C | GRY | 2704 | Reference Signal-5 Volt-MAP Sensor

#### Mass Air Flow (MAF) Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 492 | MAF sensor input
B | BLK/WHT | 451 | Ground
C | PNK | 339 | Ignition 1 feed

#### Secondary Air Injection Pump

Connector Part Information |

• | 12191968

• | 2 Way F Metric-Pack 280 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 78 | Secondary Air Injection Pump Control Circuit
B | BLK | 450 | Ground

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 12110192

• | 3-Way F Metri-Pack 150 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 2701 | 5-volt reference A
B | BLK | 2752 | TP ground
C | DK BLU | 417 | TP sensor signal

#### Transaxle Range Switch C1

Connector Part Information |

• | 12129840

• | 7-Way F Metri-Pack Mixed Series Sealed (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 434 | PARK/NEUTRAL input
B | ORN | 840 | Fused battery feed
C | LT GRN | 275 | Transaxle range switch feed-PARK
D | BLK/WHT | 451 | PCM ground
E | ORN/BLK | 1786 | Starter solenoid feed
F | LT GRN | 24 | Backup lamp feed
G | PNK | 439 | Ignition switched battery feed-START

#### Transaxle Range Switch C2

Connector Part Information |

• | 12191757

• | 4-Way F Metri-Pack 150 Series Sealed (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 776 | Transaxle range switch parity input
B | YEL | 772 | Transaxle range switch input B
C | GRY | 773 | Transaxle range switch input C
D | BLK/WHT | 771 | Transaxle range switch input A

#### Vehicle Speed Sensor (VSS)

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 401 | VSS low
B | YEL | 400 | VSS high