For 1990-2009 cars

Caution: This vehicle is equipped with a Supplemental Inflatable Restraint (SIR) System. Failure to follow the correct procedure could cause the following conditions:

• | Air bag deployment

• | Personal injury

• | Unnecessary SIR system repairs

In order to avoid the above conditions, observe the following guidelines:

• | Refer to SIR Component Views in order to determine if you are performing service on or near the SIR components or the SIR wiring.

• | If you are performing service on or near the SIR components or the SIR wiring, disable the SIR system. Refer to Disabling the SIR System.

• | The ignition switch is turned OFF.

• | The battery is disconnected.

Many service procedures require that the following components be disconnected from the deployment loops in order to avoid an accidental deployment:

• | The AIR BAG-1 fuse

• | The inflator module circuits