For 1990-2009 cars

### Removal Procedure

1. Remove the IP ashtray. Refer to Ashtray Replacement .
2. Unscrew the IP cigarette lighter housing from the cigarette lighter element.
3. Remove the IP cigarette lighter from the ashtray.

### Installation Procedure

1. Install the IP cigarette lighter to the ashtray.
2. Screw the IP cigarette lighter housing into the cigarette lighter element.
3. Install the IP ashtray. Refer to Ashtray Replacement .