For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Road test the vehicle in order to verify the customer concern. Important: It may be necessary to compare the results of the road test to a similar vehicle that is operating properly. Does the vehicle ride too hard? | -- | Go to Step 2 | System OK
2 | Inspect the tires for the proper inflation pressure. Refer to Tire Inflation Pressure Specifications in Maintenance and Lubrication. Is the tire inflation pressure correct? | -- | Go to Step 4 | Go to Step 3
3 | Inflate the tires to the correct pressure. Did you complete the repair? | -- | Go to Step 4 | --
4 |

1. Inspect the vehicle trim height. Refer to Trim Height Inspection .
2. Repair as necessary.

Did you complete the procedure?

--

Go to Step 5

--

5 | Inspect the following suspension components for wear or damage.

• | Springs

• | Struts

• | Shock Absorbers

Refer to Suspension Strut and Shock Absorber Testing - On Vehicle .

Are any of the components worn or damaged?

--

Go to Step 6

Go to Step 7

6 | Replace all of the worn or damaged components. Refer to the following procedures:

• | Strut, Strut Component, and Spring Replacement in Front Suspension

• | Shock Absorber Replacement in Rear Suspension

• | Lower Control Arm Replacement in Rear Suspension

Did you complete the repair?

--

Go to Step 7

--

7 |

1. Inspect the automatic level control system, if equipped. Refer to Automatic Level Control System Operation Check in Automatic Level Control.
2. Repair as necessary.

Did you complete the procedure?

--

Go to Step 1

--