For 1990-2009 cars

### Removal Procedure

1. Remove the push-pin retainers from the rear seat back finish panel with a flat bladed tool.
2. Remove the outer portion of the push-pin retainer from the seat back finish panel.
3. Remove the seat back finish panel from the seat back.

### Installation Procedure

1. Install the seat back finish panel to the seat back.
2. Install the outer portion of the push-pin retainer to the seat back finish panel.
3. Install the push-pin retainer until it locks into place.