For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door lock. Refer to Sliding Door Rear Lock Replacement .
2. Disconnect the wiring harness connector from the sliding door lock actuator.
3. Drill out the sliding door lock actuator rivets.
4. Remove the sliding door lock actuator from the sliding door lock.

### Installation Procedure

1. Install the sliding door lock actuator to the sliding door lock.
2. Install the rivets that attach the sliding door lock actuator.
3. Connect the wiring harness connector to the sliding door lock actuator.
4. Install the sliding door lock. Refer to Sliding Door Rear Lock Replacement .