For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector (2) from the brake fluid level sensor (1).
2. Remove the fluid level sensor (1). Use needle nose pliers in order to compress the switch locking tabs at the outboard side of the master cylinder.

### Installation Procedure

1. Place the brake fluid level sensor (1) into the reservoir, press into place to secure the sensor retaining tabs.
2. Connect the electrical connector to the brake fluid level sensor (1).