For 1990-2009 cars

### Removal Procedure

1. Open the sliding door half way.
2. Remove the bolt for the sliding door catch with the reinforcement channel from the sliding door lower track.
3. Remove the sliding door catch with the reinforcement channel from the sliding door lower track.

### Installation Procedure

1. Install the sliding door catch with reinforcement channel to the sliding door lower track.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the sliding door catch with reinforcement channel bolt to the sliding door lower track.

Tighten
Tighten the reinforcement channel bolt to 12 N·m (106 lb in).

3. Completely open the sliding door in order to ensure that the sliding door catch holds the sliding door in the open position.
4. Close the sliding door.