For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the front door window. Refer to Front Side Door Window Replacement .
4. Use a small flat-bladed tool in order to unsnap the front door window clips.
5. Remove the front door window clips from the front door window.

### Installation Procedure

1. Align the clip holes in the window.
2. Squeeze the front door window clip together onto the window.
3. Install the front door window. Refer to Front Side Door Window Replacement .
4. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install the front door trim panel. Refer to Door Trim Panel Replacement .