For 1990-2009 cars

### Removal Procedure

1. Remove the left side instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.
2. Cut the plastic tie strap securing the tape retract module to the wire harness.
3. Disconnect the tape retract module electrical connector.
4. Remove the tape retract module (1) from the vehicle.

### Installation Procedure

1. Install the tape retract module (1) to the vehicle.
2. Connect the tape retract module electrical connector.
3. Secure the tape retract module to the wire harness with a plastic tie strap.
4. Install the left side instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.