For 1990-2009 cars

Condition | Cause | Action
--- | --- | ---
The power sliding door does not power unlatch/open when the open/close switch is pressed. The door may power open if the door is manually unlatched. | The following conditions may prevent the unlatch actuator from activating:

• | Circuit 750 and/or circuit 2910 is open.

• | The unlatch actuator is defective.

The following conditions may prevent the unlatch actuator and rod from unlatching or opening the door:

• | The sliding door is locked.

• | The front rod adjustment is too long.

• | The unlatch actuator is defective.

1. Perform the Diagnostic Mode 3. Refer to Diagnostic Modes in Power Sliding Door (PSD) Diagnostic Information . Perform the indicated corrective action.
2. Complete one of the following actions:

• | Unlock the door.

• | Adjust the front rod. Refer to Sliding Door Lock Rod Adjustment .

• | Perform the Diagnostic Mode 3. Refer to Diagnostic Modes in Power Sliding Door (PSD) Diagnostic Information . Perform the indicated corrective action.

The following conditions exist:

• | The PSD unlatches but does not power open when you press the open/close switch.

• | The PSD does not power open if you move the door manually.

There is an electrical malfunction within the PSD system.

Refer to Power Sliding Door (PSD) Diagnostic System Check .

One of the following conditions exists:

• | The PSD unlatches but does not power open when you press the open/close switch. The PSD power opens if you move the door manually.

• | The PSD does not power open when you activate the handle. The PSD power opens when you move the door manually.

• | There is a malfunction in the detent switch circuit.

• | The door lock rod is out of adjustment.

• | An electric noise is present.

• | Adjust the door lock rods. Refer to Sliding Door Lock Rod Adjustment .

• | Repair the electric noise:

- | Verify that the pads and plungers are securely attached to the body and the door. Replace the pouch fastener, as needed.

- | Inspect for corrosion, water entry, and dirty or sticking plungers. Clean or replace the plungers as needed.

- | Inspect the ground circuits.

- | Inspect the detent switch. Replace the detent switch as needed. Refer to Rear Latch Detent Switch - Power Sliding Door.

If these steps do not correct the condition, refer to Power Sliding Door (PSD) Diagnostic System Check .

The PSD reverses or stops during a power opening. |

• | There is a mechanical obstruction.

• | The cable tension is incorrect.

1. Complete the following steps in order to clear the mechanical obstruction as needed:

• | Remove any foreign objects. Clean or replace the track, as needed.

• | Inspect the roller brackets for binding. Adjust the lower track. Use lithium grease in order to lubricate the lower track at the bend.

• | Inspect the roller brackets for wear. Replace the brackets as needed.

2. Adjust the cable tension. Refer to Cable Tension Adjustment - Sliding Door (Regular Method) for regular method or Cable Tension Adjustment - Sliding Door (Alternate Method) for atlernate method in Doors.

If these steps do not correct the condition, refer to Power Sliding Door (PSD) Diagnostic System Check .

The sliding door does not remain open when the vehicle is on a hill (incline or decline). |

• | The cable tension is incorrect.

• | The hold open system is faulty.

• | Adjust the cable tension. Refer to Cable Tension Adjustment - Sliding Door (Regular Method) for regular method or Cable Tension Adjustment - Sliding Door (Alternate Method) for atlernate method in Doors.

• | Adjust, clean, or replace the hold open spring/retainer.

If these steps do not correct the condition, refer to Power Sliding Door (PSD) Diagnostic System Check .