For 1990-2009 cars

1. Remove the steering column tilt head assembly. Refer to Steering Column Tilt Head Housing - Disassemble - Off Vehicle .
2. Slide the PASSKEY® III (2) off of the electronic lock module assembly (1).
3. Remove the key alarm connector (1) from the electronic lock module assembly (2).
4. Remove the two tapping screws from the ignition key alarm switch assembly (3).
5. Let both parts hang freely.
6. Remove the park lock cable assembly (1) from the electronic lock module assembly.
7. Remove the three pan head tapping screws (2) from the electronic lock module assembly (1).
8. Remove the electronic lock module assembly (1).