For 1990-2009 cars

## Roof Console Replacement Single

### Removal Procedure

1. Insert a small, flat-bladed tool between the interior lamp/multifunction switch/reading lamp housing and the overhead console.
2. Press inward and down in order to release the interior lamp/multifunction switch/reading lamp housing from the overhead console.
3. Remove the interior lamp/multifunction switch/reading lamp housing from the overhead console.
4. Disconnect the electrical connectors from the interior lamp/multifunction switch.
5. Remove the headliner. Refer to Headlining Trim Panel Replacement .
6. Remove the screw from the rear of the overhead console.
7. Remove the locking nuts from the locating posts.
8. Remove the overhead console from the headliner.
9. Remove the push-nut retainer from the overhead console post in order to separate the 2 halves of the overhead console (single storage).

### Installation Procedure

1. Install the push-in retainer to the overhead console post to keep the 2 halves of the overhead console together (single storage).
2. Press the overhead console into the headliner.
3. Install the locking nuts to the locating posts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the screw to the rear of the overhead console.

Tighten
Tighten the screw to 2 N·m (18 lb in).

5. Install the headliner. Refer to Headlining Trim Panel Replacement .
6. Connect the electrical connectors to the interior lamp/multifunction switch.
7. Align the retaining tabs on the interior lamp/multifunction switch/reading lamp housing with the overhead console.
8. Press up on the interior lamp/multifunction switch/reading lamp housing in order to press the housing into the overhead console.

## Roof Console Replacement Dual

### Removal Procedure

1. Insert a small, flat-bladed tool between the interior lamp/multifunction switch/reading lamp housing and the overhead console.
2. Press inward and down in order to release the interior lamp/multifunction switch/reading lamp housing from the overhead console.
3. Remove the interior lamp/multifunction switch/reading lamp housing from the overhead console.
4. Disconnect the electrical connectors from the interior lamp/multifunction switch.
5. Remove the screw from the front of the overhead console.
6. Open the rear storage compartment in the overhead console in order to access the rear screws.
7. Remove the screws from the rear of the front overhead console.
8. Remove the overhead console from the headliner.
9. Remove the driver information center. Refer to Driver Information Center Replacement in Instrument Panel, Gauges and Console.

### Installation Procedure

1. Install the driver information center. Refer to Driver Information Center Replacement in Instrument Panel, Gages and Console.
2. Align the overhead console to the headliner.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screw to the front of the overhead console.

Tighten
Tighten the screw to 2 N·m (18 lb in).

4. Open the rear storage compartment in the overhead console in order to access the holes for the rear mounting screws.
5. Install the screws to the rear of the overhead console.

Tighten
Tighten the screw to 2 N·m (18 lb in).

6. Connect the electrical connectors to the interior lamp/multifunction switch.
7. Align the retaining tabs on the interior lamp/multifunction switch/reading lamp housing with the overhead console.
8. Press up on the interior lamp/multifunction switch/reading lamp housing in order to install the housing into the overhead console.

## Roof Console Replacement CF5

### Removal Procedure

1. Insert a small, flat-bladed tool between the interior lamp/multifunction switch/reading lamp housing and the overhead console.
2. Press inward and down in order to release the interior lamp/multifunction switch/reading lamp housing from the overhead console.
3. Remove the interior lamp/multifunction switch/reading lamp housing from the overhead console.
4. Disconnect the electrical connectors from the interior lamp/multifunction switch.
5. Use a flat-bladed tool in order to unsnap the retainers from the overhead console bracket.
6. Remove the overhead console from the headliner.

### Installation Procedure

1. Install the overhead console to the headliner.
2. Install the overhead console retainers into the overhead console bracket.
3. Connect the electrical connectors to the interior lamp/multifunction switch.
4. Align the retaining tabs on the interior lamp/multifunction switch/reading lamp housing with the overhead console.
5. Press up on the interior lamp/multifunction switch/reading lamp housing in order to install the housing into the overhead console.