For 1990-2009 cars

### Removal Procedure

1. Drain Cooling system. Refer to Cooling System Draining and Filling in Engine Cooling.
2. Remove the wiper module cover.
3. Remove the air cleaner duct and cover. Refer to Air Filter Element Replacement in Engine Controls -- 3.4L.
4. Rotate the engine forward and secure. Refer to Rotating the Engine for Service Access in Engine Mechanical.
5. Disconnect the inlet pipe to auxiliary coolant pump hose from the inlet pipe.
6. Disconnect the inlet pipe to auxiliary coolant pump hose from the auxiliary coolant pump (4).
7. Remove the inlet pipe to auxiliary coolant pump hose (3).

### Installation Procedure

1. Install the inlet pipe to auxiliary coolant pump hose (3).
2. Connect the inlet pipe to auxiliary coolant pump hose to the auxiliary coolant pump (4).
3. Connect the inlet pipe to auxiliary coolant pump hose to the inlet pipe.
4. Rotate the engine rearward to the proper position. Refer to Rotating the Engine for Service Access in Engine Mechanical.
5. Install the air cleaner cover and duct. Refer to Air Filter Element Replacement in Engine Controls -- 3.4L.
6. Install the wiper module cover.
7. Refill the cooling system. Refer to Cooling System Draining and Filling in Engine Cooling.