For 1990-2009 cars

### Removal Procedure

1. Using a small, flat-bladed tool, remove the coat hook access hole cover from the roof side rail lamp.
2. Remove the screws from the roof side rail lamp.
3. Remove the roof side rail lamp from the roof.
4. Disconnect the electrical connectors from the roof side rail lamp.

### Installation Procedure

1. Connect the electrical connectors to the roof side rail lamp.
2. Install the roof side rail lamp to the roof.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screws to the roof side rail lamp.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Snap the coat hook access hole cover back into place on the roof side rail lamp.