For 1990-2009 cars

### Installation Procedure

#### Tools Required

• | J 28467-B Universal Engine Support Fixture

• | J 28467-500 Engine Support Fixture

1. Remove the right side engine mount strut. Refer to Engine Mount Strut Replacement .
2. Install the J 28467-500 .
3. Install the spreader bar to the engine mount strut bracket.
4. Install the spreader bar to the engine right side engine lift hook.
5. Install the J 28467-6A .
6. Install the J 28467-7A to the engine left side engine lift hook.
7. Install the J 28467-34 .
8. Install the J 28467-6A .
9. Install the J 28467-8A to the spreader bar.
10. Install the J 28467-34 .
11. The engine support fixture upper portion installed.

Important: Perform the following steps only if you are disconnecting both of the powertrain mounts from the frame or the powertrain.

12. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.

Caution: The utility straps MUST be installed in order to prevent forward movement of the powertrain. If the utility straps are not installed, the powertrain will move which may cause personal injury and vehicle damage.

13. Install the J 28467-500UPD to the engine.
14. Install the J 28467-500UPD opposite end to the underbody rail.
15. Install the OTHER J 28467-500UPD to the transaxle.
16. Install the J 28467-500UPD opposite end to the underbody rail.
17. Tighten both of the J 28467-500UPD utility straps in order to prevent forward movement of the powertrain.

### Removal Procedure

1. Remove both of the J 28467-500UPD .
2. Lower the vehicle.
3. Remove the J 28467-34 .
4. Remove the J 28467-7A .
5. Remove the J 28467-6A .
6. Remove the J 28467-34 .
7. Remove the J 28467-8A .
8. Remove the J 28467-6A .
9. Remove the J 28467-500 .
10. Install the right side engine mount strut. Refer to Engine Mount Strut Replacement .