For 1990-2009 cars

1. Install the oil dam (27) into the case.
2. Assemble the manual valve link onto the manual shift detent lever/IMS detent lever.
3. Connect the manual valve link (402) to the manual valve (404).
4. Install the manual valve link spring (403).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the manual shift detent assembly (804), and the manual shift detent bolt (805).

Tighten
Tighten the bolt to 12 N·m (106 lb in).

6. Carefully install the input speed sensor (440) into the case cover (400).
7. Install the input speed sensor clip (441) into the case cover (400).