For 1990-2009 cars

## Rear SeatAudio Control Replacement Pontiac

### Removal Procedure

1. Use a small, flat-bladed tool in order to press on the locking tabs and release the rear seat audio controls from the rear overhead console.
2. Disconnect the electrical connectors.
3. Remove the rear seat audio controls from the rear overhead console.

### Installation Procedure

1. Connect the electrical connectors to the rear seat audio controls.
2. Align the rear seat audio controls to the rear overhead console.
3. Press the rear seat audio controls into the rear overhead console until fully seated and locked in.

## Rear SeatAudio Control Replacement Oldsmobile

### Removal Procedure

1. Carefully release the locking tabs using a flat-bladed tool in the locations as indicated.
2. Remove the rear seat audio from the overhead entertainment console.
3. Disconnect the electrical connector from the rear seat audio.

### Installation Procedure

1. Connect the electrical connector to the rear seat audio.
2. Install the rear seat audio to the overhead entertainment console.
3. Press the rear seat audio until it locks into place.