For 1990-2009 cars

Condition | Action
--- | ---
Air exists in the power steering system. | Bleed the power steering system. Refer to Power Steering System Bleeding .
The steering column intermediate shaft is loose. | Repair or replace the steering column intermediate shaft. Refer to Lower/Upper Intermediate Steering Shaft Replacement in Steering Wheel and Column.
The steering gear is loose. | Tighten the steering gear bolts to specification. Refer to Steering Gear Replacement .
The tie rod end(s) are loose. | Repair or replace the tie rod ends as necessary. Refer to Rack and Pinion Outer Tie Rod End Replacement .
The wheel bearing/hub is loose. | Repair or replace the wheel bearing/hub. Refer to Front Wheel Bearing and Hub Replacement In Front Suspension.
There is excessive play in the steering. | Refer to Too Much Play in Steering .