For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
1-2 Shift Solenoid (1-2 SS) Valve | Inside the automatic transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | --
2-3 Shift Solenoid (2-3 SS) Valve | Inside the automatic transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | --
A/C Compressor Clutch Coil | Part of the A/C compressor, right side of engine at the end of the crankshaft, near the crankshaft position sensor (24x) | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
A/C Refrigerant Pressure Sensor | Left side of the engine compartment, below the accumulator, below the air cleaner assembly | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Air Injection Bleed Valve | Left rear of engine, above valve cover | -- | Engine Controls Connector End Views
AIR Pump Relay | Forward lamp harness, right side of the engine compartment, rearward of the Horn | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Automatic Transaxle Fluid Temperature (TFT) Sensor | Inside the automatic transaxle | -- | Shift Lock Control Connector End Views in Automatic Transaxle-4T65E
Bank 1 Knock Sensor (KS) | Front of the engine, above the starter | Engine Controls Component Views | Engine Controls Connector End Views
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Camshaft Position (CMP) Sensor | Engine compartment, right side of the engine, above the A/C compressor clutch | Engine Controls Component Views | Engine Controls Connector End Views
Cool Fan 1 Relay | Engine compartment, in the underhood accessory wiring junction block | -- | --
Cool Fan 2 Relay | Engine compartment, in the underhood accessory wiring junction block | -- | --
Cool Fan Relay | Engine compartment, in the underhood accessory wiring junction block | -- | --
Crank Relay | Right side of Engine Compartment on the radiator support, inboard of the underhood accessory wiring junction block | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Crankshaft Position (CKP) Sensor (7X) | Lower rear of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Crankshaft Position (CKP) Sensor (24X) | Right side of the engine, at the end of the crankshaft, behind the harmonic balancer | Engine Controls Component Views | Engine Controls Connector End Views
Cruise Control Module | Engine compartment, near the left strut tower | Cruise Control Component Views in Cruise Control | Cruise Control Connector End Views in Cruise Control
Cruise Control Release Switch | Mounted to the brake pedal support | Cruise Control Component Views in Cruise Control | Cruise Control Connector End Views in Cruise Control
Cruise Control Switch | Part of the turn signal switch, on the turn signal lever | Theft Deterrent System Component Views in Theft Deterrent | Cruise Control Connector End Views in Cruise Control
Data Link Connector (DLC) | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Electronic Brake Control Module (EBCM) | Lower left side of the engine compartment | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
Engine Coolant Fan Motor 1 (RH) | Mounted to the rear left side of the radiator | Cooling System Component Views in Engine Cooling | Cooling System Connector End Views in Engine Cooling
Engine Coolant Fan Motor 2 (LH) | Mounted to the rear right side of the radiator | Cooling System Component Views in Engine Cooling | Cooling System Connector End Views in Engine Cooling
Engine Coolant Level Indicator Module | Mounted to the rear right side of the radiator, below the radiator cap | Cooling System Component Views in Engine Cooling | Cooling System Connector End Views in Engine Cooling
Engine Coolant Temperature (ECT) Sensor | Left side top of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Engine Oil Level Indicator Switch | Center of the engine oil pan | Engine Controls Component Views | Engine Controls Connector End Views
Engine Oil Pressure Indicator Switch | Front of the engine, above the starter | Engine Controls Component Views | Engine Controls Connector End Views
Evaporative Emissions (EVAP) Canister Purge Solenoid Valve | Top rear of the engine, below the ignition control module | Engine Controls Component Views | Engine Controls Connector End Views
Evaporative Emissions (EVAP) Canister Vent Solenoid Valve | Below the center of the vehicle, forward of the fuel tank | Engine Controls Component Views | Engine Controls Connector End Views
Exhaust Gas Recirculation (EGR) Valve | Upper left side of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Injectors | Top of the engine at each cylinder intake port | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Level Sender | Mounted inside the fuel tank | -- | --
Fuel Pump Motor | Mounted inside the fuel tank | -- | --
Fuel Pump Relay | Engine compartment, in the underhood accessory wiring junction block | -- | --
Fuel Tank | Below the left side, middle of the vehicle | -- | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | Electrical Center Identification Views in Wiring Systems
Fusible Link A | Bolted to the starter solenoid | -- | --
Fusible Link C | Bolted to the starter solenoid | -- | --
Fusible Link K | Bolted to the starter solenoid | -- | --
Fusible Link Z | Bolted to the starter solenoid | -- | --
Generator | Top rear right side of the engine | Engine Electrical Component Views in Engine Electrical | Engine Electrical Connector End Views in Engine Electrical
Heated Oxygen Sensor 1 (HO2S 1) | Rear of the engine, in the exhaust manifold | Engine Controls Component Views | Engine Controls Connector End Views
Heated Oxygen Sensor 2 (HO2S 2) | In the exhaust system, behind the catalytic converter | Engine Controls Component Views | Engine Controls Connector End Views
Heater-A/C Control | Center of the IP, below the radio | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Heater-A/C Control (Blower Motor Switch) | Part of the heater-A/C control | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Idle Air Control (IAC) Valve | Top of the engine, front of the throttle assembly | Engine Controls Component Views | Engine Controls Connector End Views
Ignition Control Module (ICM) | Top center rear of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Ignition Switch | Part of the steering column | -- | --
Instrument Cluster | Left side of the IP | Engine Controls Component Views in Instrument Panel, Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Intake Air Temperature (IAT) Sensor | Left of engine compartment, on the air intake duct, near the throttle body | Engine Controls Component Views | Engine Controls Connector End Views
Manifold Absolute Pressure (MAP) Sensor | Right top of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Mass Air Flow (MAF) Sensor | Left front of the engine compartment, in the air cleaner duct | Engine Controls Component Views | Engine Controls Connector End Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Rear Side Door Actuator Motor | Right quarter panel, above the wheelhouse | Power Door Systems Component Views in Doors | --
Rear Side Door Actuator Motor (Optical Sensor) | Part of the rear side door actuator motor | Power Door Systems Component Views in Doors | --
Relay Center | Right side of IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Secondary Air Injection Pump | Mounted in lower portion of the drivers front fender | -- | Engine Controls Connector End Views
Splice Pack SP205 | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Starter Motor | Lower front of the engine | -- | --
Starter Solenoid | Lower front of the engine, part of the starter motor assembly | -- | --
Stop Lamp Switch | Mounted to the brake pedal support | Cruise Control Component Views in Cruise Control | Lighting Systems Connector End Views in Lighting Systems
Throttle Position (TP) Sensor | Top of the engine, on the throttle assembly | Engine Controls Component Views | Engine Controls Connector End Views
Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM SOL) Valve | Inside the automatic transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | --
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Engine Controls Component Views | Automatic Transmission Related Connector End Views in Automatic Transaxle-4T65-E
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Vehicle Speed Sensor (VSS) | Lower right rear of the engine compartment, mounted to the right side of the transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | Automatic Transmission Related Connector End Views in Automatic Transaxle-4T65-E
C101 (20 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, near the EBCM | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C102 (16 cavities) | Engine wiring harness to the fuel injector wiring harness, top of the engine, near the generator next to C108 | -- | Inline Harness Connector End Views in Wiring Systems
C105 (4 cavities) | Engine wiring harness to the engine coolant fan wiring harness, behind the engine coolant fan 1 (left) | -- | Inline Harness Connector End Views in Wiring Systems
C111 (14 cavities) | Engine wiring harness to the automatic transaxle wiring harness, lower left side of the engine compartment, front of the automatic transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | Automatic Transmission Inline Harness Connector End View in Automatic Transaxle-4T65-E
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C305 (12 cavities) | Body wiring harness to the electronic brake control wiring harness and fuel sender wiring harness, mounted as a pass through, beneath the vehicle behind the driver seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G101 | Front of the vehicle, right of the left headlamp, on the front upper crossmember | -- | --
G111 | Engine compartment, left of the starter, along with the battery ground | Harness Routing Views in Wiring Systems | --
G113 | Engine compartment, left of the starter, along with the battery ground | Harness Routing Views in Wiring Systems | --
G114 | Engine compartment, left and above the starter, near the starter solenoid | Harness Routing Views in Wiring Systems | --
G117 | Engine compartment, left and above the starter, near the starter solenoid | Harness Routing Views in Wiring Systems | --
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in Wiring Systems | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views in Wiring Systems | --
S105 | Engine harness, top right side radiator approximately 20 cm (8 in) from the engine coolant fan 1 (right) motor breakout | -- | --
S106 | Engine harness, front left side of the engine compartment approximately 10 cm (4 in) from the PCM breakout | -- | --
S108 | Engine harness, front left side of the engine compartment approximately 8 cm (3 in) from the PCM breakout | -- | --
S109 | Fuel injector harness, center of the engine approximately 16 cm (6 in) from C102 | -- | --
S110 | Fuel injector harness, center of the engine approximately 14 cm (4 in) from C102 | -- | --
S167 | Engine harness, front left side of the engine approximately 5 cm (2 in) PCM breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S210 | IP harness, center of the IP approximately 4 cm (2 in) from the security indicator lamp breakout | -- | --
S211 | IP harness, left side of the IP approximately 15 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S238 | IP harness, center of the IP approximately 80 cm (31 in) from the cigar lighter connector | -- | --
S264 | IP harness, right side of the IP approximately 16 cm (6 in) from the relay center breakout | -- | --
S329 | Fuel sender harness, between C305 and the fuel tank approximately 20 cm (8 in) from C305 | -- | --