For 1990-2009 cars

## Automatic Level Control Inflator Air Switch Replacement VIN U

### Removal Procedure

1. Remove the inflator air valve opening cover by pulling the lever inboard.
2. Remove the inflator control access panel retainers.
3. Disconnect the electrical connector from the inflator switch.
4. Remove the switch from the inflator control panel by depressing the retainers on the inflator switch.

### Installation Procedure

1. Install the inflator switch to the inflator control panel snaps into place.
2. Connect the electrical connectors to the inflator switch.
3. Install the inflator control access panel retainers.
4. Install the inflator air valve opening cover by pushing the lever outboard.

## Automatic Level Control Inflator Air Switch Replacement VIN X w/ C34

### Removal Procedure

1. Remove the inflator air valve opening cover by pulling the lever inboard.
2. Remove the inflator control access panel retainers.
3. Disconnect the electrical connector from the inflator switch.
4. Remove the switch from the inflator control panel by depressing the retainers on the inflator switch.

### Installation Procedure

1. Install the inflator switch to the inflator control panel snaps into place.
2. Connect the electrical connectors to the inflator switch.
3. Install the inflator control access panel retainers.
4. Install the inflator air valve opening cover by pushing the lever outboard.

## Automatic Level Control Inflator Air Switch Replacement VIN X w/o C34

### Removal Procedure

1. Remove the inflator air valve opening cover by pulling the lever inboard.
2. Remove the inflator control access panel retainers.
3. Disconnect the electrical connector from the inflator switch.
4. Remove the switch from the inflator control panel by depressing the retainers on the inflator switch.

### Installation Procedure

1. Install the inflator switch to the inflator control panel snaps into place.
2. Connect the electrical connectors to the inflator switch.
3. Install the inflator control access panel retainers.
4. Install the inflator air valve opening cover by pushing the lever outboard.