For 1990-2009 cars

Abbreviation | Material Name | Heat Resisting Temperature °C (°F) | Resistance to Gasoline and Solvents | Other Cautions
--- | --- | --- | --- | ---
AAS | Acrylonitrile acrylic rubber styrene | 95 (203) | Avoid gasoline and solvents | Avoid brake fluid
ABS | Acrylonitrile butadiene-styrene resin | 90 (194) | Avoid gasoline and solvents | Avoid brake fluid
AES | Acrylonitrile ethylene styrene | 90 (194) | Avoid gasoline and solvents | Avoid brake fluid
FRP | Fiber reinforced plastics | 170 (338) | Gasoline and most solvents are harmless | --
PA, PAG, PAGG | Polyamide (nylon) | 150 (302) | Gasoline and most solvents are harmless | Avoid immersing in water
PBT | Polybutylene terephthalate | 140 (284) | Gasoline and most solvents are harmless | --
PC | Polycarbonate | 120 (248) | Avoid gasoline and solvents | --
PE | Polyethylene | 80 (176) | Gasoline and most solvents are harmless | Flammable
PMMA | Polymethyl methacrylate | 90 (194) | Avoid gasoline and solvents | Avoid brake fluid
POM | Polyacetal | 120 (248) | Gasoline and most solvents are harmless | Avoid battery acid
PP | Polypropylene | 90 (194) | Gasoline and most solvents are harmless | Flammable
PPC | Polypropylene composite | 115 (239) | Gasoline and most solvents are harmless | Flammable
PPE | Polyphenylene ether | 110 (230) | Avoid gasoline and solvents | --
PUR | Polyurethane | 90 (194) | Gasoline and most solvents are harmless | Avoid brake fluid
PVC | Polyvinyl chloride | 90 (194) | Gasoline and most solvents are harmless if wiped up quickly | Toxic when burned
TPE | Thermoplastic elastomer | 80 (176) | Avoid gasoline and solvents | --
TPR | Thermoplastic rubber | 80 (176) | Avoid gasoline and solvents | --