For 1990-2009 cars

### Removal Procedure

1. Slide the rear seat to the most rearward position.
2. Fold the seat back so its flat.
3. Pull the strap on the back side of the rear seat riser in order to release the riser from the floor.
4. Tilt the rear seat fully upwards.
5. Lift the rear seat from the latch.
6. Remove the rear seat from the vehicle.

### Installation Procedure

1. Install the rear seat to the vehicle.
2. Secure the front seat riser latches into the floor.

Ensure that the latch is secured on both pins.

3. Tilt the rear seat assembly down and latch the rear seat riser latches into the floor.
4. Tilt the rear seat back upright.
5. Return the rear seat to its original position.