For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Door Trim Panel Replacement .
2. Route the electrical harness through the water deflector.
3. Peel off the water deflector from the inner door.

### Installation Procedure

1. Route the electrical harness through the water deflector.

Important: Proper adhesive bonding of the front door water deflector to the inner panel is critical in order to prevent water leaks.

2. Position the water deflector to the inner door.
3. Press the water deflector onto the inner door.
4. Install the front door trim panel. Refer to Door Trim Panel Replacement .