For 1990-2009 cars

### Removal Procedure

1. Insert a small, flat-bladed tool between the interior lamp/multifunction switch/reading lamp housing and the overhead console.
2. Press inward and down in order to release the interior lamp/multifunction switch/reading lamp housing from the overhead console.
3. Remove the interior lamp/multifunction switch/reading lamp housing from the overhead console.
4. Disconnect the electrical connectors from the interior lamp/multifunction switch.
5. Remove the interior lamp/multifunction switch by using pliers in order to compress the interior lamp/multifunction switch retainers while pulling switch away from the housing.

### Installation Procedure

1. Install the interior lamp/multifunction switch into the interior lamp/multifunction switch/reading lamp housing.
2. Connect the electrical connectors to the interior lamp/multifunction switch.
3. Align the retaining tabs on the interior lamp/multifunction switch/reading lamp housing with the overhead console
4. Press up on the interior lamp/multifunction switch/reading lamp housing in order to install the housing into the overhead console.