For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
2. Disconnect the electrical connector to the air inlet valve electric actuator.
3. Remove the mounting screws from the air inlet valve electric actuator.
4. Remove the air inlet valve electric actuator.

### Installation Procedure

1. Install the air inlet valve electric actuator.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the mounting screws to the air inlet valve electric actuator.

Tighten
Tighten the screws to 1.6 N·m (14 lb in).

3. Connect the electrical connector to the air inlet valve electric actuator.
4. Install the instrument panel compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.