For 1990-2009 cars

### Removal Procedure

1. Remove the rear storage compartment. Refer to Rear Storage Compartment Replacement in Interior Trim.
2. Pull the alarm (4) from power sliding door actuator motor, separating the hook and loop retainer.
3. Remove the alarm electrical connector.

### Installation Procedure

1. Connect the alarm electrical connector.
2. Push the alarm (4) onto the power sliding door actuator motor, securing the hook and loop retainer.
3. Install the rear storage compartment. Refer to Rear Storage Compartment Replacement in Interior Trim.