For 1990-2009 cars

### Removal Procedure

1. Remove the throttle body air inlet duct. Refer to Air Filter Element Replacement in Engine Controls - 3.4L.
2. Remove the engine mount struts. Refer to Engine Mount Strut Replacement .
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
4. Remove the three-way catalytic converter pipe from the engine right side exhaust manifold. Refer to Catalytic Converter Replacement in Engine Exhaust.
5. Remove the right front wheel and tire. Refer to Tire and Wheel Removal and Installation
6. Remove the right engine splash shield. Refer to Engine Splash Shield Replacement in Body Front End.
7. Remove the engine mount lower nuts.

Notice: In order to avoid oil pan damage and possible engine failure, insert a block of wood that spans the width of the oil pan bottom between the oil pan and the jack support.

8. Use a utility stand and a block of wood in order to raise the engine.
9. Remove the engine mount bracket-to-oil pan bolts.
10. Remove the engine mount and the engine mount bracket.
11. Remove the engine mount upper nuts.
12. Remove the engine mount from the engine mount bracket.

### Installation Procedure

1. Install the engine mount to the engine mount bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the engine mount upper nuts.

Tighten
Tighten the engine mount upper nuts to 47 N·m (35 lb ft).

3. Install the engine mount bracket with the engine mount to the oil pan.
4. Install the engine mount bracket-to-oil pan bolts.

Tighten
Tighten the engine mount bracket-to-oil pan bolts to 58 N·m (43 lb ft).

5. Use the utility stand in order to lower the engine.
6. Install the engine mount lower nuts.

Tighten
Tighten the engine mount lower nuts to 43 N·m (32 lb ft).

7. Install the right engine splash shield. Refer to Engine Splash Shield Replacement in Body Front End.
8. Install the right front wheel and tire. Refer to Tire and Wheel Removal and Installation
9. Connect the three-way catalytic converter pipe to the engine right side exhaust manifold. Refer to Catalytic Converter Replacement in Engine Exhaust.
10. Lower the vehicle.
11. Install the engine mount struts. Refer to Engine Mount Strut Replacement .
12. Install the throttle body air inlet duct. Refer to Air Filter Element Replacement in Engine Controls - 3.4L.