For 1990-2009 cars

### Removal Procedure

1. Remove the head restraint. Refer to Front Seat Head Restraint Replacement .
2. Remove the seat back cover. Refer to Front Seat Back Cushion Cover Replacement .
3. Remove the seat back pad. Refer to Front Seat Back Cushion Pad Replacement .
4. Squeeze the bottom of the head restraint guide together and pull the head restraint guide from the seat back frame.

### Installation Procedure

1. Push the head restraint guide into the seat back frame. Make sure it locks into place.
2. Install the seat back pad. Refer to Front Seat Back Cushion Pad Replacement .
3. Install the seat back cover. Refer to Front Seat Back Cushion Cover Replacement .
4. Install the head restraint. Refer to Front Seat Head Restraint Replacement .